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ESKOM HOLDINGS SOC Ltd		CONTRACT NUMBER _________
PROJECT AND CONTRACT TITLE		


TSC3 	PAGE 1 OF 43 	COVER PAGE
PART C1 	PAGE 1 OF 2 	AGREEMENTS & CONTRACT DATA

C1.1 Form of Offer & Acceptance

[bookmark: _Toc231466156][bookmark: _Toc231566405][bookmark: _Toc231566524][bookmark: _Toc231566644][bookmark: _Toc231566764][bookmark: _Toc231567027][bookmark: _Toc231567179][bookmark: _Toc233624188]Offer

The Employer, identified in the Acceptance signature block, has solicited offers to enter into a contract for the procurement of:

[bookmark: _Toc231466157][bookmark: _Toc231566406][bookmark: _Toc231566525][bookmark: _Toc231566645][bookmark: _Toc231566765][bookmark: _Toc231567028][bookmark: _Toc231567180][bookmark: _Toc233624189]The provision of Gardening Services at Drakensberg for a period of 5 years

The tenderer, identified in the Offer signature block, has examined the documents listed in the Tender Data and addenda thereto and by submitting this Offer has accepted the Conditions of Tender.

By the representative of the tenderer, deemed to be duly authorised, signing this part of this Form of Offer and Acceptance the tenderer offers to perform all of the obligations and liabilities of the Contractor under the contract including compliance with all its terms and conditions according to their true intent and meaning for an amount to be determined in accordance with the conditions of contract identified in the Contract Data. 

Delete the row for the Options which do not apply
	Options A 
	The offered total of the Prices exclusive of VAT is 
	R [●]

	
	Sub total
	R [●]

	
	Value Added Tax @ 15% is
	R [●]

	
	The offered total of the amount due inclusive of VAT is[footnoteRef:1] [1:  This total is required by the Employer for budgeting purposes only.  Actual amounts due will be assessed in terms of the conditions of contract.] 

	R [●]

	
	(in words) [●]




This Offer may be accepted by the Employer by signing the Acceptance part of this Form of Offer and Acceptance and returning one copy of this document including the Schedule of Deviations (if any) to the tenderer before the end of the period of validity stated in the Tender Data, or other period as agreed, whereupon the tenderer becomes the party named as the Contractor in the conditions of contract identified in the Contract Data.

	Signature(s)

	
	
	

	Name(s)

	
	
	

	Capacity

	
	
	

	For the tenderer:

	

	
Name & signature of witness
	(Insert name and address of organisation)



	
	

Date
	

	
Tenderer’s CIDB registration number: 
	



[bookmark: _Toc231466158][bookmark: _Toc231566407][bookmark: _Toc231566526][bookmark: _Toc231566646][bookmark: _Toc231566766][bookmark: _Toc231567029][bookmark: _Toc231567181][bookmark: _Toc233624190]
Acceptance

By signing this part of this Form of Offer and Acceptance, the Employer identified below accepts the tenderer’s Offer.  In consideration thereof, the Employer shall pay the Contractor the amount due in accordance with the conditions of contract identified in the Contract Data.  Acceptance of the tenderer’s Offer shall form an agreement between the Employer and the tenderer upon the terms and conditions contained in this agreement and in the contract that is the subject of this agreement.

The terms of the contract, are contained in: 

Part C1		Agreements and Contract Data, (which includes this Form of Offer and Acceptance)

Part C2		Pricing Data

Part C3		Scope of Work: Service Information

and drawings and documents (or parts thereof), which may be incorporated by reference into the above listed Parts.

Deviations from and amendments to the documents listed in the Tender Data and any addenda thereto listed in the Returnable Schedules as well as any changes to the terms of the Offer agreed by the tenderer and the Employer during this process of offer and acceptance, are contained in the Schedule of Deviations attached to and forming part of this Form of Offer and Acceptance.  No amendments to or deviations from said documents are valid unless contained in this Schedule.

The tenderer shall within two weeks of receiving a completed copy of this agreement, including the Schedule of Deviations (if any), contact the Employer’s agent (whose details are given in the Contract Data) to arrange the delivery of any securities, bonds, guarantees, proof of insurance and any other documentation to be provided in terms of the conditions of contract identified in the Contract Data at, or just after, the date this agreement comes into effect.  Failure to fulfil any of these obligations in accordance with those terms shall constitute a repudiation of this agreement.

Notwithstanding anything contained herein, this agreement comes into effect on the date when the tenderer receives one fully completed and signed original copy of this document, including the Schedule of Deviations (if any).  


	Signature(s)

	
	
	

	Name(s)
	

	
	

	Capacity

	
	
	

	for the Employer

	

	
Name & signature of witness
	(Insert name and address of organisation)
	
	

Date
	



Note: If a tenderer wishes to submit alternative tenders, use another copy of this Form of Offer and Acceptance.
[bookmark: _Toc231466159][bookmark: _Toc231566408][bookmark: _Toc231566527][bookmark: _Toc231566647][bookmark: _Toc231566767][bookmark: _Toc231567030][bookmark: _Toc231567182][bookmark: _Toc233624191]
Schedule of Deviations to be completed by the Employer prior to contract award
Note:
1.  This part of the Offer & Acceptance would not be required if the contract has been developed by negotiation between the Parties and is not the result of a process of competitive tendering.
2. The extent of deviations from the tender documents issued by the Employer prior to the tender closing date is limited to those permitted in terms of the Conditions of Tender.
3. A tenderer’s covering letter must not be included in the final contract document.  Should any matter in such letter, which constitutes a deviation as aforesaid be the subject of agreement reached during the process of Offer and Acceptance, the outcome of such agreement shall be recorded here and the final draft of the contract documents shall be revised to incorporate the effect of it.

	No.
	Subject
	Details

	1
	[●]
	[●]

	2
	[●]
	[●]

	3
	[●]
	[●]

	4
	[●]
	[●]

	5
	[●]
	[●]

	6
	[●]
	[●]

	7
	[●]
	[●]

	
	
	




By the duly authorised representatives signing this Schedule of Deviations below, the Employer and the tenderer agree to and accept this Schedule of Deviations as the only deviations from and amendments to the documents listed in the Tender Data and any addenda thereto listed in the Tender Schedules, as well as any confirmation, clarification or changes to the terms of the Offer agreed by the tenderer and the Employer during this process of Offer and Acceptance.  

It is expressly agreed that no other matter whether in writing, oral communication or implied during the period between the issue of the tender documents and the receipt by the tenderer of a completed signed copy of this Form shall have any meaning or effect in the contract between the parties arising from this Agreement. 


	
	For the tenderer:

	
	For the Employer


	Signature

	
	
	

	Name
	

	
	Maremane Tsotetsi

	Capacity

	
	
	Middle Manager Plant Management

	On behalf of
	(Insert name and address of organisation)



	
	Eskom Holdings SOC Ltd
Drakensberg Pumped Storage Scheme

	Name & signature of witness
	
	
	

	
Date
	
	
	





ESKOM HOLDINGS SOC Ltd.		CONTRACT NUMBER ______________
TITLE OF PROJECT /CONTRACT		



PART C1 AGREEMENTS AND CONTRACT DATA	PAGE 2 OF 5 	C.1.1 FORM OF OFFER AND ACCEPTANCE

C1.2 TSC3 Contract Data

[bookmark: _Toc231466160][bookmark: _Toc231566409][bookmark: _Toc231566528][bookmark: _Toc231566648][bookmark: _Toc231566768][bookmark: _Toc231567031][bookmark: _Toc231567183][bookmark: _Toc233624192]Part one - Data provided by the Employer


Completion of this data in full, according to the Options chosen, is essential to create a complete contract.

	Clause
	[bookmark: _Toc231466161][bookmark: _Toc231566410][bookmark: _Toc231566529][bookmark: _Toc231566649][bookmark: _Toc231566769][bookmark: _Toc231567032][bookmark: _Toc231567184][bookmark: _Toc233624193]Statement
	[bookmark: _Toc231466162][bookmark: _Toc231566411][bookmark: _Toc231566530][bookmark: _Toc231566650][bookmark: _Toc231566770][bookmark: _Toc231567033][bookmark: _Toc231567185][bookmark: _Toc233624194]Data

	1
	[bookmark: _Toc231466163][bookmark: _Toc231566412][bookmark: _Toc231566531][bookmark: _Toc231566651][bookmark: _Toc231566771][bookmark: _Toc231567034][bookmark: _Toc231567186][bookmark: _Toc233624195]General
	

	
	The conditions of contract are the core clauses and the clauses for main Option: 
	

	
	
	A:	Priced contract with price list

	
	dispute resolution Option
	W1:	Dispute resolution procedure

	
	and secondary Options
	

	
	
	X1:	Price adjustment for inflation

	
	
	X2	Changes in the law

	
	
	X17:	Low service damages

	
	
	X18:	Limitation of liability

	
	
	X19:	Task Order

	
	
	Z:		Additional conditions of contract

	
	of the NEC3 Term Service Contract April 2013[footnoteRef:2] (TSC3) [2:  Available from Engineering Contract Strategies Tel 011 803 3008 Fax 086 539 1902 www.ecs.co.za ] 

	If 2005 Edition is to be used delete “April 2013” and replace with “June 2005 with amendments June 2006”. Always delete this note before finalising this Data

	10.1
	The Employer is (name):
	Eskom Holdings SOC Ltd (reg no: 2002/015527/30), a state owned company incorporated in terms of the company laws of the Republic of South Africa

	
	Address
	Registered office at Megawatt Park, Maxwell Drive, Sandton, Johannesburg

	10.1
	The Service Manager is (name): 
	Jenelle Kumar

	
	Address
	Drakensberg Pumped Storage Scheme, Jagersrust, 3354

	
	Tel
	036 342 3396

	
	e-mail
	KumarJN@eskom.co.za

	11.2(2)
	The Affected Property is
	Drakensberg Pumped Storage Scheme & Jagersrust Village (including access roads)

	11.2(13)
	The service is 
	The Provision of Gardening Services 

	

	
	

	11.2(14)
	The following matters will be included in the Risk Register
	None

	11.2(15)
	The Service Information is in 
	Part 3: Scope of Work and all documents and drawings to which it makes reference.

	12.2
	The law of the contract is the law of 
	the Republic of South Africa

	13.1
	The language of this contract is 
	English

	13.3
	The period for reply is
	· Immediately for health and safety matters 
· 1 week during planning phase 
· Three (3) working days during execution phase 

	[bookmark: _Toc231466164][bookmark: _Toc231566413][bookmark: _Toc231566532][bookmark: _Toc231566652][bookmark: _Toc231566772][bookmark: _Toc231567035][bookmark: _Toc231567187][bookmark: _Toc233624196]2
	[bookmark: _Toc231466165][bookmark: _Toc231566414][bookmark: _Toc231566533][bookmark: _Toc231566653][bookmark: _Toc231566773][bookmark: _Toc231567036][bookmark: _Toc231567188][bookmark: _Toc233624197]The Contractor’s main responsibilities
	Data required by this section of the core clauses is also provided by the Contractor in Part 2 and terms in italics used in this section are identified elsewhere in this Contract Data

	21.1
	The Contractor submits a first plan for acceptance within
	
Two (2) weeks of the Contract Date

	[bookmark: _Toc231466166][bookmark: _Toc231566415][bookmark: _Toc231566534][bookmark: _Toc231566654][bookmark: _Toc231566774][bookmark: _Toc231567037][bookmark: _Toc231567189][bookmark: _Toc233624198]3
	[bookmark: _Toc231466167][bookmark: _Toc231566416][bookmark: _Toc231566535][bookmark: _Toc231566655][bookmark: _Toc231566775][bookmark: _Toc231567038][bookmark: _Toc231567190][bookmark: _Toc233624199]Time
	

	30.1
	The starting date is.
	TBC

	30.1
	The service period is
	Five (5) years 

	[bookmark: _Toc231466168][bookmark: _Toc231566417][bookmark: _Toc231566536][bookmark: _Toc231566656][bookmark: _Toc231566776][bookmark: _Toc231567039][bookmark: _Toc231567191][bookmark: _Toc233624200]4
	[bookmark: _Toc231466169][bookmark: _Toc231566418][bookmark: _Toc231566537][bookmark: _Toc231566657][bookmark: _Toc231566777][bookmark: _Toc231567040][bookmark: _Toc231567192][bookmark: _Toc233624201]Testing and defects
	[bookmark: _Toc231466170][bookmark: _Toc231566419][bookmark: _Toc231566538][bookmark: _Toc231566658][bookmark: _Toc231566778][bookmark: _Toc231567041][bookmark: _Toc231567193][bookmark: _Toc233624202]There is no reference to Contract Data in this section of the core clauses and terms in italics used in this section are identified elsewhere in this Contract Data

	[bookmark: _Toc231466171][bookmark: _Toc231566420][bookmark: _Toc231566539][bookmark: _Toc231566659][bookmark: _Toc231566779][bookmark: _Toc231567042][bookmark: _Toc231567194][bookmark: _Toc233624203]5
	[bookmark: _Toc231466172][bookmark: _Toc231566421][bookmark: _Toc231566540][bookmark: _Toc231566660][bookmark: _Toc231566780][bookmark: _Toc231567043][bookmark: _Toc231567195][bookmark: _Toc233624204]Payment
	

	50.1
	The assessment interval is 
	between the 25th - 30th day of each successive month or Completion of Task Order. 

	51.1
	The currency of this contract is the 
	South African Rand

	51.2
	The period within which payments are made is
	30 days from when the Contractor provides the Employer with an invoice in accordance with the law of the contract and the Employer's requirements stated in the Z Clauses and/or Services   Information, reflecting the amount due for payment equal to that certified, accepted, or corrected by the Service Manager,  or decided by the Adjudicator or awarded by the tribunal, as applicable.

	51.4
	The interest rate is 

	the publicly quoted prime rate of interest (calculated on a 365 day year) charged by from time to time by the Standard Bank of South Africa Limited (as certified, in the event of any dispute, by any manager of such bank, whose appointment it shall not be necessary to prove) for amounts due in Rands and 

(ii) the LIBOR rate applicable at the time for amounts due in other currencies.  LIBOR is the 6 month London Interbank Offered Rate quoted under the caption “Money Rates” in The Wall Street Journal for the applicable currency or if no rate is quoted for the currency in question then the rate for United States Dollars, and  if no such rate appears in The Wall Street Journal then the rate as quoted by the Reuters Monitor Money Rates Service (or such service as may replace the Reuters Monitor Money Rates Service) on the due date for the payment in question, adjusted mutatis mutandis every 6 months thereafter (and as certified, in the event of any dispute, by any manager employed in the foreign exchange department of The Standard Bank of South Africa Limited, whose appointment it shall not be necessary to prove.

	[bookmark: _Toc231466173][bookmark: _Toc231566422][bookmark: _Toc231566541][bookmark: _Toc231566661][bookmark: _Toc231566781][bookmark: _Toc231567044][bookmark: _Toc231567196][bookmark: _Toc233624205]6
	[bookmark: _Toc231466174][bookmark: _Toc231566423][bookmark: _Toc231566542][bookmark: _Toc231566662][bookmark: _Toc231566782][bookmark: _Toc231567045][bookmark: _Toc231567197][bookmark: _Toc233624206]Compensation events
	There is no reference to Contract Data in this section of the core clauses and terms in italics used in this section are identified elsewhere in this Contract Data.

	[bookmark: _Toc231466175][bookmark: _Toc231566424][bookmark: _Toc231566543][bookmark: _Toc231566663][bookmark: _Toc231566783][bookmark: _Toc231567046][bookmark: _Toc231567198][bookmark: _Toc233624207]7
	[bookmark: _Toc231466176][bookmark: _Toc231566425][bookmark: _Toc231566544][bookmark: _Toc231566664][bookmark: _Toc231566784][bookmark: _Toc231567047][bookmark: _Toc231567199][bookmark: _Toc233624208]Use of Equipment Plant and Materials
	[bookmark: _Toc231466177][bookmark: _Toc231566426][bookmark: _Toc231566545][bookmark: _Toc231566665][bookmark: _Toc231566785][bookmark: _Toc231567048][bookmark: _Toc231567200][bookmark: _Toc233624209]There is no reference to Contract Data in this section of the core clauses and terms in italics used in this section are identified elsewhere in this Contract Data.

	[bookmark: _Toc231466178][bookmark: _Toc231566427][bookmark: _Toc231566546][bookmark: _Toc231566666][bookmark: _Toc231566786][bookmark: _Toc231567049][bookmark: _Toc231567201][bookmark: _Toc233624210]8
	[bookmark: _Toc231466179][bookmark: _Toc231566428][bookmark: _Toc231566547][bookmark: _Toc231566667][bookmark: _Toc231566787][bookmark: _Toc231567050][bookmark: _Toc231567202][bookmark: _Toc233624211]Risks and insurance
	

	80.1
	These are additional Employer's risks  
	1. Risks for activities will be dealt with task specific procedures.

	[bookmark: _Toc231466180][bookmark: _Toc231566429][bookmark: _Toc231566548][bookmark: _Toc231566668][bookmark: _Toc231566788][bookmark: _Toc231567051][bookmark: _Toc231567203][bookmark: _Toc233624212]9
	[bookmark: _Toc231466181][bookmark: _Toc231566430][bookmark: _Toc231566549][bookmark: _Toc231566669][bookmark: _Toc231566789][bookmark: _Toc231567052][bookmark: _Toc231567204][bookmark: _Toc233624213]Termination
	There is no reference to Contract Data in this section of the core clauses and terms in italics used in this section are identified elsewhere in this Contract Data.

	[bookmark: _Toc231466182][bookmark: _Toc231566431][bookmark: _Toc231566550][bookmark: _Toc231566670][bookmark: _Toc231566790][bookmark: _Toc231567053][bookmark: _Toc231567205][bookmark: _Toc233624214]10
	[bookmark: _Toc231466183][bookmark: _Toc231566432][bookmark: _Toc231566551][bookmark: _Toc231566671][bookmark: _Toc231566791][bookmark: _Toc231567054][bookmark: _Toc231567206][bookmark: _Toc233624215]Data for main Option clause
	

	A
	Priced contract with price list
	

	20.5
	The Contractor prepares forecasts of the final total of the Prices for the whole of the service at intervals no longer than 
	

2 weeks.

	[bookmark: _Toc231466184][bookmark: _Toc231566433][bookmark: _Toc231566552][bookmark: _Toc231566672][bookmark: _Toc231566792][bookmark: _Toc231567055][bookmark: _Toc231567207][bookmark: _Toc233624216]11
	[bookmark: _Toc231466185][bookmark: _Toc231566434][bookmark: _Toc231566553][bookmark: _Toc231566673][bookmark: _Toc231566793][bookmark: _Toc231567056][bookmark: _Toc231567208][bookmark: _Toc233624217]Data for Option W1
	

	W1.1
	The Adjudicator 
	the person selected from the ICE-SA Division (or its successor body) of the South African Institution of Civil Engineering Panel of Adjudicators by the Party intending to refer a dispute to him.  (see www.ice-sa.org.za). If the Parties do not agree on an Adjudicator the Adjudicator will be appointed by the Arbitration Foundation of Southern Africa (AFSA).

	W1.2(3)
	The Adjudicator nominating body is: 
	the Chairman of ICE-SA a joint Division of the South African Institution of Civil Engineering and the Institution of Civil Engineers (London) (see www.ice-sa.org.za ) or its successor body.

	W1.4(2)
	The tribunal is: 
	arbitration

	W1.4(5)
	The arbitration procedure is 
	the latest edition of Rules for the Conduct of Arbitrations published by The Association of Arbitrators (Southern Africa) or its successor body.

	
	The place where arbitration is to be held is
	KwaZulu Natal, South Africa

	
	The person or organisation who will choose an arbitrator 
· if the Parties cannot agree a choice or
· if the arbitration procedure does not state who selects an arbitrator, is
	

the Chairman for the time being or his nominee of the Association of Arbitrators (Southern Africa) or its successor body.

	[bookmark: _Toc231466186][bookmark: _Toc231566435][bookmark: _Toc231566554][bookmark: _Toc231566674][bookmark: _Toc231566794][bookmark: _Toc231567057][bookmark: _Toc231567209][bookmark: _Toc233624218]12
	[bookmark: _Toc231466187][bookmark: _Toc231566436][bookmark: _Toc231566555][bookmark: _Toc231566675][bookmark: _Toc231566795][bookmark: _Toc231567058][bookmark: _Toc231567210][bookmark: _Toc233624219]Data for secondary Option clauses
	

	X1
	Price adjustment for inflation
	

	X1.1
	The base date for indices is 
	One month before tender closure. Rates are fixed and firm for the first 12 months. 

	
	The proportions used to calculate the Price Adjustment Factor are:
	proportion
	linked to index for
	Index prepared by

	
	
	0.85
	CPI
	SEIFSA

	
	
	0.15
	Fixed/non-adjustable
	

	
	
	1.00
	
	

	
	
	The proportions used to calculate the Price Adjustment Factor are:
SEIFSA
· 15% fixed
· 85% variable for which: 
70% SEIFSA C-3 Actual Labour Cost
15% SEIFSA L-1(B) Own Transport of         Goods and Personnel
15% SEIFSA D-2 Consumer Price Index

	 
	CPA frequency:                                           Semi‑annual (6 months)

	X2
	Changes in the law
	There is no reference to Contract Data in this Option and terms in italics are identified elsewhere in this Contract Data.

	X17
	Low service damages
	

	X17.1
	The service level table is 

	Low Service Damage Description 

	Value Of Low Service Damages 
	Limit Of Low Service Damage 

	Lawn maintenance 
Failure to cut grass to specified height and/or width. 
	1.5% of Task order value per week
	Limited to 10% of task order value

	Hedge and shrub trimming 
Failure to trim hedges/shrubs as specified
	1.5% of Task order value per week
	Limited to 10% of task order value

	General appearance 
Garden areas not kept tidy (tools left, uneven finish, unsafe conditions)
	1.5% of Task order value per week
	Limited to 10% of task order value

	Contractor’s Health and Safety file:
Submission of SHE file two (2) weeks before start of work. Also, at intervals as required by the Employer’s Safety Department.
	1.5% of Task order value per week
	Limited to 10% of task order value

	Submission Delays:
Delays in submission of documents as detailed in this agreement
	
2% of Task order value per week
	
Limited to 10% of task order value

	Delay damages:
Delays in completing the Task as per Task Order programme 
	
2% of Task order value per week

	
Limited to 10% of task order value

	Resource delay 
Delays in providing minimum resources as per Contract requirements
	
2% of Task order value per week
	
Limited to 10% of task order value




	X18
	Limitation of liability
	

	X18.1
	The Contractor’s liability to the Employer for indirect or consequential loss is limited to
	

R0.0 (zero Rand)

	X18.2
	For any one event, the Contractor’s liability to the Employer for loss of or damage to the Employer’s property is limited to
	the amount of the deductibles relevant to the event 

	[bookmark: OLE_LINK1][bookmark: OLE_LINK2]X18.3
	The Contractor’s liability for Defects due to his design of an item of Equipment is limited to
	The greater of 

the total of the Prices at the Contract Date
and 
the amounts excluded and unrecoverable from the Employer’s insurance (other than the resulting physical damage to the Employer’s property which is not excluded) plus the applicable deductibles

	X18.4
	The Contractor’s total liability to the Employer, for all matters arising under or in connection with this contract, other than the excluded matters, is limited to
	the total of the Prices other than for the additional excluded matters.

The Contractor’s total liability for the additional excluded matters is not limited. 

The additional excluded matters are amounts for which the Contractor is liable under this contract for

Defects due to his design, plan and specification,
Defects due to manufacture and fabrication outside the Affected Property, 
loss of or damage to property (other than the Employer’s property, Plant and Materials),
death of or injury to a person and
infringement of an intellectual property right.

	X18.5
	The end of liability date is 
	12 months after the end of the service period.

	X19
	Task Order
	

	X19.5
	The Contractor submits a Task Order programme to the Service Manager within 
	
Three (3) days of receiving the Task Order

	Z
	The additional conditions of contract are
	
Z1 to Z14 always apply.

	
	

	Z1
	Cession delegation and assignment

	Z1.1
	The Contractor does not cede, delegate or assign any of its rights or obligations to any person without the written consent of the Employer.

	Z1.2
	Notwithstanding the above, the Employer may on written notice to the Contractor cede and delegate its rights and obligations under this contract to any of its subsidiaries or any of its present divisions or operations which may be converted into separate legal entities as a result of the restructuring of the Electricity Supply Industry. 

	
	

	Z2
	Joint ventures

	Z2.1
	If the Contractor constitutes a joint venture, consortium or other unincorporated grouping of two or more persons or organisations then these persons or organisations are deemed to be jointly and severally liable to the Employer for the performance of this contract.

	Z2.2
	Unless already notified to the Employer, the persons or organisations notify the Service Manager within two weeks of the Contract Date of the key person who has the authority to bind the Contractor on their behalf.

	Z2.3
	The Contractor does not alter the composition of the joint venture, consortium or other unincorporated grouping of two or more persons without the consent of the Employer having been given to the Contractor in writing.

	
	

	Z3
	Change of Broad Based Black Economic Empowerment (B-BBEE) status

	Z3.1
	Where a change in the Contractor’s legal status, ownership or any other change to his business composition or business dealings results in a change to the Contractor’s B-BBEE status, the Contractor notifies the Employer within seven days of the change.

	Z3.2
	The Contractor is required to submit an updated verification certificate and necessary supporting documentation confirming the change in his B-BBEE status to the Service Manager within thirty days of the notification or as otherwise instructed by the Service Manager.

	Z3.3
	Where, as a result, the Contractor’s B-BBEE status has decreased since the Contract Date the Employer may either re-negotiate this contract or alternatively, terminate the Contractor’s obligation to Provide the Service.

	Z3.4
	Failure by the Contractor to notify the Employer of a change in its B-BBEE status may constitute a reason for termination. If the Employer terminates in terms of this clause, the procedures on termination are P1, P2 and P4 as stated in clause 92, and the amount due is A1 and A3 as stated in clause 93.

	
	

	Z4
	Confidentiality

	Z4.1
	The Contractor does not disclose or make any information arising from or in connection with this contract available to Others. This undertaking does not, however, apply to information which at the time of disclosure or thereafter, without default on the part of the Contractor, enters the public domain or to information which was already in the possession of the Contractor at the time of disclosure (evidenced by written records in existence at that time).  Should the Contractor disclose information to Others in terms of clause 25.1, the Contractor ensures that the provisions of this clause are complied with by the recipient.

	Z4.2
	If the Contractor is uncertain about whether any such information is confidential, it is to be regarded as such until notified otherwise by the Service Manager.

	Z4.3
	In the event that the Contractor is, at any time, required by law to disclose any such information which is required to be kept confidential, the Contractor, to the extent permitted by law prior to disclosure, notifies the Employer so that an appropriate protection order and/or any other action can be taken if possible, prior to any disclosure.  In the event that such protective order is not, or cannot, be obtained, then the Contractor may disclose that portion of the information which it is required to be disclosed by law and uses reasonable efforts to obtain assurances that confidential treatment will be afforded to the information so disclosed.

	Z4.4
	The taking of images (whether photographs, video footage or otherwise) of the Affected Property or any portion thereof, in the course of Providing the Service and after the end of the service period, requires the prior written consent of the Service Manager.  All rights in and to all such images vests exclusively in the Employer.  

	Z4.5
	The Contractor ensures that all his subcontractors abide by the undertakings in this clause.

	
	

	Z5
	Waiver and estoppel: Add to core clause 12.3:

	Z5.1
	Any extension, concession, waiver or relaxation of any action stated in this contract by the Parties, the Service Manager or the Adjudicator does not constitute a waiver of rights, and does not give rise to an estoppel unless the Parties agree otherwise and confirm such agreement in writing.

	
	

	Z6
	Health, safety and the environment:  Add to core clause 27.4

	Z6.1
	The Contractor undertakes to take all reasonable precautions to maintain the health and safety of persons in and about the execution of the service. Without limitation the Contractor:
Complies with the Occupational Health and Safety Act 85 of 1993 and all applicable health, safety and environmental laws and regulations;
Complies with all Employer health, safety and environmental rules, procedures and site requirements;
warrants that the total of the Prices as at the Contract Date includes a sufficient amount for proper compliance with all applicable health, safety and environmental laws and regulations and the health and safety rules, guidelines and procedures provided for in this contract and generally for the proper maintenance of health & safety in and about the execution of the service; and
undertakes, in and about the execution of the service, to comply with all applicable health, safety and environmental laws and regulations and rules, guidelines and procedures otherwise provided for under this contract and ensures that his Subcontractors, employees and others under the Contractor’s direction and control, likewise observe and comply with the foregoing.
Maintains all required safety documentation, certifications and compliance records necessary for the execution of the service.

	Z6.2
	The Contractor, in and about the execution of the service, complies with all applicable environmental laws and regulations and rules, guidelines and procedures otherwise provided for under this contract and ensures that his Subcontractors, employees and others under the Contractor’s direction and control, likewise observe and comply with the foregoing.

	
	

	Z7
	Provision of a tax invoice, payment and interest 

	
Z7.1
	The Contractor (if registered in South Africa in terms of the Companies Act) is required to comply with the requirements of the Value Added Tax Act, (Act 89 of 1991 (as amended)) and to include the Employer’s VAT number 4740101508 on each invoice submitted for payment.

	Z7.2
	Within one week of receiving a payment certificate from the  Service Manager or the Employer’s acceptance or correction of  the Contractor’s assessment or application for payment, the Contractor provides the Employer with a tax invoice in the form required by the law of the contract, and this contract, including in accordance with any requirements and procedures stated in the Service Information, and showing the amount due for payment equal to that stated in the payment certificate, or that accepted or corrected assessment or application for payment.

	Z7.3
	If the Contractor does not provide a tax invoice in the form to be legally compliant, reflecting the certified, accepted or corrected amount and by the time required by this contract, the time by when the Employer is to make a payment, and the date from which interest is assessed for the certified, accepted or corrected amount, is extended by a period equal in time to the delayed submission of the legally compliant tax invoice.

	Z7.4




Z7.5
	The Contractor’s provision of a tax invoice reflecting the certified, accepted or corrected amount does not affect the Parties’ rights in terms of this contract, including with respect to disputed amounts.

The Contractor at all times complies with Employer’s Vendor Management System requirements to ensure invoices are processed and paid timeously. It is the Contractor’s responsibility to ensure that the Employer is informed of any changes in its organisation that would affect its vendor status, and to ensure that the necessary actions and due diligences are taken to ensure compliance with the Employer’s Vendor Management System. The Employer will not be liable for a delay in payment of invoices as a result of the Contractor’s non-compliant status on the Employer’s Vendor Management System and no interest will be claimable in this instance.

	Z8
	Notifying compensation events

	Z8.1
	Delete the last paragraph of core clause 61.3 and replace with:

If the Contractor does not notify a compensation event within eight weeks of becoming aware of the event, he is not entitled to a change in the Prices.

	[bookmark: OLE_LINK5][bookmark: OLE_LINK6]Z9
	Employer’s limitation of liability

	Z9.1
	The Employer’s liability to the Contractor for the Contractor’s indirect or consequential loss is limited to R0.00 (zero Rand)

	Z9.2
	The Contractor’s entitlement under the indemnity in 82.1 is provided for in 60.1(12) and the Employer’s liability under the indemnity is limited to compensation as provided for in core clause 63 and X19.11 if Option X19 Task Order applies to this contract. 

	
	

	Z10
	Termination: Add to core clause 91.1, at the second main bullet point, fourth sub-bullet point, after the words "against it":  

	Z10.1
	   or had a business rescue order granted against it.

	
	

	Z11
	Ethics

	For the purposes of this Z-clause, the following definitions apply:

	Affected Party
	means, as the context requires, any party, irrespective of whether it is the Contractor or a third party, such party’s employees, agents, or Subcontractors or Subcontractor’s employees, or any one or more of all of these parties’ relatives or friends,

	Coercive Action
	means to harm or threaten to harm, directly or indirectly, an Affected Party or the property of an Affected Party, or to otherwise influence or attempt to influence an Affected Party to act unlawfully or illegally,

	Collusive Action
	means where two or more parties co-operate to achieve an unlawful or illegal purpose, including to influence an Affected Party to act unlawfully or illegally,

	Committing Party
	means, as the context requires, the Contractor, or any member thereof in the case of a joint venture, or its employees, agents, or Subcontractors or the Subcontractor’s employees,

	Corrupt Action
	means the offering, giving, taking, or soliciting, directly or indirectly, of a good or service to unlawfully or illegally influence the actions of an Affected Party,

	Fraudulent Action
	means any unlawfully or illegally intentional act or omission that misleads, or attempts to mislead, an Affected Party, in order to obtain a financial or other benefit or to avoid an obligation or incurring an obligation,

	Obstructive Action
	means a Committing Party unlawfully or illegally destroying, falsifying, altering or concealing information or making false statements to materially impede an investigation into allegations of Prohibited Action, and

	Prohibited Action
	means any one or more of a Coercive Action, Collusive Action Corrupt Action, Fraudulent Action or Obstructive Action.

	Z11.1
	A Committing Party may not take any Prohibited Action during the course of the procurement of this contract or in execution thereof.

	Z11.2
	The Employer may terminate the Contractor’s obligation to Provide the Services if a Committing Party has taken such Prohibited Action and the Contractor did not take timely and appropriate action to prevent or remedy the situation, without limiting any other rights or remedies the Employer has. It is not required that the Committing Party had to have been found guilty, in court or in any other similar process, of such Prohibited Action before the Employer can terminate the Contractor’s obligation to Provide the Services for this reason.

	Z11.3
	If the Employer terminates the Contractor’s obligation to Provide the Services for this reason, the amounts due on termination are those intended in core clauses 92.1 and 92.2.

	Z11.4
	A Committing Party co-operates fully with any investigation pursuant to alleged Prohibited Action. Where the Employer does not have a contractual bond with the Committing Party, the Contractor ensures that the Committing Party co-operates fully with an investigation.




Z12		Insurance

Z 12.1	Replace core clause 83 with the following:

	Insurance cover
	83
	

	
	83.1
	When requested by a Party, the other Party provides certificates from his insurer or broker stating that the insurances required by this contract are in force.


	
	83.2
	The Contractor provides the insurances stated in the Insurance Table A from the starting date until the earlier of Completion and the date of the termination certificate. 



	
INSURANCE TABLE A
	Insurance against
	Minimum amount of cover or minimum limit of indemnity

	Loss of or damage caused by the Contractor to the Employer’s property
	The replacement cost where not covered by the Employer’s insurance.

The Employer’s policy deductible as at Contract Date, where covered by the Employer’s insurance.

	Loss of or damage to Plant and Materials
	The replacement cost where not covered by the Employer’s insurance.

The Employer’s policy deductible as at Contract Date, where covered by the Employer’s insurance.

	Loss of or damage to Equipment
	The replacement cost where not covered by the Employer’s insurance.

The Employer’s policy deductible as at Contract Date, where covered by the Employer’s insurance.

	The Contractor’s liability for loss of or damage to property (except the Employer’s property, Plant and Materials and Equipment) and liability for bodily injury to or death of a person (not an employee of the Contractor) arising from or in connection with the Contractor’s Providing the Service
	Loss of or damage to property
The replacement cost

Bodily injury to or death of a person
The amount required by the applicable law.

	Liability for death of or bodily injury to employees of the Contractor arising out of and in the course of their employment in connection with this contract
	The amount required by the applicable law








Z 12.2	Replace core clause 86 with the following:
	Insurance by the Employer
	86
	


	
	86.1
	The Employer provides the insurances stated in the Insurance Table B

	
	
	

	
	
	INSURANCE TABLE B

	Insurance against or name of policy
	Minimum amount of cover or minimum limit of indemnity

	Assets All Risk
	Per the insurance policy document

	Contract Works insurance
	Per the insurance policy document

	Environmental Liability
	Per the insurance policy document

	General and Public Liability
	Per the insurance policy document

	Transportation (Marine)
	Per the insurance policy document

	Motor Fleet and Mobile Plant
	Per the insurance policy document

	Terrorism
	Per the insurance policy document

	Cyber Liability
	Per the insurance policy document

	Nuclear Material Damage and Business Interruption
	Per the insurance policy document

	Nuclear Material Damage Terrorism
	Per the insurance policy document






	Z13
	Intellectual Property – Eskom owning Intellectual Property

	“Intellectual Property”
	means (a) patents, trademarks, service marks, rights in designs, trade names, trade secrets, know how, copyrights and topography rights, in each case whether registered or not; (b) applications for registration of any of them; (c) rights under licences and consents in relation to any of them; (d) all forms of protection of a similar nature or having equivalent or similar effect to any of them which may subsist anywhere in the world.

	“Background Intellectual Property"
	means any and all Intellectual Property rights that are not Foreground Intellectual Property and are owned or controlled by the relevant party or licensed to the relevant party prior to or outside of the services but required for the purposes of the services.

	“Foreground Intellectual Property”
	means all Intellectual Property rights and other matter capable of being the subject of intellectual property rights that is conceived, first reduced to practice or writing or developed in whole or in substantial part in the course of the execution of the services and rights which are developed substantially as a result of the services.  Any services that will be developed, changed, modified and/or improved specifically for the Purposes will be Foreground Intellectual Property.  Any data or any other information relating to Employer’s proprietary information generated from the use of the Contractor’s Background Intellectual Property.

	Z13.1
	The Contractor retains ownership of all Background Intellectual Property rights made by or on behalf of the Contractor as part of the services in information or material it uses in carrying out the services.

	Z13.2
	All Foreground Intellectual Property rights, contained in any developed materials which are created by the Contractor or on behalf of the Contractor, for the purposes of and in support of the execution of the services Employer’s IP) vest with the Employer.  

	Z13.3
	Any data or any other information relating to Employer’s proprietary information generated from the use of the Contractor’s Background Intellectual Property, the copyright therein shall be owned by the Employer.

	Z13.4
	The Contractor acknowledges that all rights, title, and interest in and to the Foreground Intellectual Property that may result or originate from or be developed in execution of the services vests in the Employer and that the Contractor has no claim of any nature in and to the Foreground Intellectual Property.  

	Z13.5
	The Contractor ensures that a copyright notice is incorporated or embossed or labelled on the Foreground Intellectual Property, where the Employer is reflected as the owner of the Foreground Intellectual Property.  

	Z13.6
	The Contractor is obliged to provide Foreground Intellectual Property manufacturing documents, designs, processes and/or specifications to the Employer before/on the [completion date].

	Z13.7
	The Contractor procures that each Sub-Contractor executes all and any services and takes all and any other actions as may be required, in order to give effect to this Agreement.

	Z13.8
	The Employer retains all Background Intellectual Property rights in all documents made by or on behalf of the Employer including all documents and requirements provided prior to or during the execution of the services.  The Contractor does not, without the written consent, of the Employer, copy, use or issue to a third party any of the Employer’s Background Intellectual Property documents and requirements except for the purposes of executing the services.

	Z13.9
	Either party procures that any third party executes confidentiality undertakings not to disclose to any other third parties, any of the [Employer’s Background Intellectual Property and IP documents and requirements at all, in respect of the Employer], or the Background Intellectual Property, in respect of the Contractor.



	Z13.10
	Third Party Claims:

	Z13.10.1
	In the event of any claims being made or actions against the Employer, on the ground that the Contractor infringed any patent, trade mark or copyright, the Contractor is notified thereof and at its own expense, conducts all negotiations in consultation with the Employer for the settlement of the claim and litigation that may arise from such alleged infringement, provided that the Employer will not bear any financial burden or losses.

	Z13.10.2
	Save where the Contractor fails to take over the conduct of the negotiation or litigation within a reasonable time of the notification of the alleged infringement, the Employer does not make any admission which might be prejudicial to the Contractor’s position. The Employer, at the request and the cost of the Contractor affords it all reasonable technical assistance that the Employer is able to provide for the purpose of contesting any such claim or action.

	Z13.10.3
	Should it be held in any such action that any such protected rights have been infringed, as definitely stated by a judgment of the court before which the action is brought, the Contractor, at its own expense and in consultation with the Employer, either:
a. procures for [Employer/Client/Purchaser] the right to continue to use the affected item or design, or
b. replaces the said affected item or design with a non-infringing item, or
c. provides a design of equivalent quality or modify such affected item or design so as to make it non-infringing without affecting the quality.

	Z13.10.4
	Notwithstanding anything contained in this contract, the foregoing sets forth the entire responsibility of Contractor with respect to claims relating to infringement.

	Z13.10.5
	Where it is alleged that the Employer has committed an infringement as intended vis-à-vis the Contractor as set out in the third-party intellectual property infringement clause, the Employer has the same rights and obligations as the Contractor, mutatis mutandis, as regards such alleged infringement.

	Z13.10.6
	The Contractor herewith indemnifies the Employer and undertakes to keep the Employer indemnified against all claims of whatsoever nature, real or imagined, which may be made against the Employer arising from the infringement of any third-party intellectual property rights.

	
	

	Z14
	Asbestos

	For the purposes of this Z-clause, the following definitions apply:

	AAIA
	means approved asbestos inspection authority.

	ACM
	means asbestos containing materials.

	AL
	means action level, i.e. a level of 50% of the OEL, i.e. 0.1 regulated asbestos fibres per ml of air measured over a 4-hour period. The value at which proactive actions is required in order to control asbestos exposure to prevent exceeding the OEL.

	Ambient Air
	means breathable air in area of work with specific reference to breathing zone, which is defined to be a virtual area within a radius of approximately 30cm from the nose inlet.

	Compliance Monitoring
	means compliance sampling used to assess whether or not the personal exposure of workers to regulated asbestos fibres is in compliance with the Standard’s requirements for safe processing, handling, storing, disposal and phase-out of asbestos and asbestos containing material, equipment and articles.

	OEL
	means occupational exposure limit.

	Parallel Measurements
	means measurements performed in parallel, yet separately, to existing measurements to verify validity of results.

	Safe Levels
	means airborne asbestos exposure levels conforming to the Standard’s requirements for safe processing, handling, storing, disposal and phase-out of asbestos and asbestos containing material, equipment and articles.

	Standard
	means the Employer’s Asbestos Standard 32-303: Requirements for Safe Processing, Handling, Storing, Disposal and Phase-out of Asbestos and Asbestos Containing Material, Equipment and Articles.

	SANAS
	means the South African National Accreditation System.

	TWA
	means the average exposure, within a given workplace, to airborne asbestos fibres, normalised to the baseline of a 4-hour continuous period, also applicable to short term exposures, i.e. 10-minute TWA.

	Z14.1
	The Employer ensures that the Ambient Air in the area where the Contractor will Provide the Services conforms to the acceptable prescribed South African standard for asbestos, as per the regulations published in GNR 155 of 10 February 2002, under the Occupational Health and Safety Act, 1993 (Act 85 of 1993) (“Asbestos Regulations”). The OEL for asbestos is 0.2 regulated asbestos fibres per millilitre of air as a 4-hour TWA, averaged over any continuous period of four hours, and the short term exposure limit of 0.6 regulated asbestos fibres per millilitre of air as a 10-minute TWA, averaged over any 10 minutes, measured in accordance with HSG248 and monitored according to HSG173 and OESSM.

	Z14.2
	Upon written request by the Contractor, the Employer certifies that these conditions prevail. All measurements and reporting are effected by an independent, competent, and certified occupational hygiene inspection body, i.e. a SANAS accredited and Department of Employment and Labour approved AAIA. The Contractor may perform Parallel Measurements and related control measures at the Contractor’s expense. For the purposes of compliance the results generated from Parallel Measurements are evaluated only against South African statutory limits as detailed in clause Z14.1. Control measures conform to the requirements stipulated in the AAIA-approved asbestos work plan.

	Z14.3
	The Employer manages asbestos and ACM according to the Standard.

	Z14.4
	In the event that any asbestos is identified while Providing the Services, a risk assessment is conducted and if so required, with reference to possible exposure to an airborne concentration of above the AL for asbestos, immediate control measures are implemented and relevant air monitoring conducted in order to declare the area safe.

	Z14.5
	The Contractor’s personnel are entitled to stop working and leave the contaminated area forthwith until such time that the area of concern is declared safe by either Compliance Monitoring or an AAIA approved control measure intervention, for example, per the emergency asbestos work plan, if applicable.

	Z14.6
	The Contractor continues to Provide the Services, without additional control measures presented on presentation of Safe Levels. The contractually agreed dates to Provide the Services, including the Completion Date, are adjusted accordingly. The contractually agreed dates are extended by the notification periods required by regulations 3 and 21 of the Asbestos Regulations, 2001.

	Z14.7
	Any removal and disposal of asbestos, asbestos containing materials and waste, is done by a registered asbestos contractor, instructed by the Employer at the Employer’s expense, and conducted in line with South African legislation.
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C1.2 Contract Data

[bookmark: _Toc231466188][bookmark: _Toc231566437][bookmark: _Toc231566556][bookmark: _Toc231566676][bookmark: _Toc231566796][bookmark: _Toc231567059][bookmark: _Toc231567211][bookmark: _Toc233624220]Part two - Data provided by the Contractor


Notes to a tendering contractor:

1. Please read both the both the NEC3 Term Service Contract April 2013 and the relevant parts of its Guidance Notes (TSC3-GN)[footnoteRef:3] in order to understand the implications of this Data which the tenderer is required to complete. [3:  Available from Engineering Contract Strategies Tel 011 803 3008 Fax 086 5391902 or www.ecs.co.za ] 

2. The number of the clause which requires the data is shown in the left hand column for each statement however other clauses may also use the same data.
3. [bookmark: Text530]Where a form field like this [     ] appears, data is required to be inserted relevant to the option selected. Click on the form field once and type in the data.  Otherwise complete by hand and in ink.

Completion of the data in full, according to Options chosen, is essential to create a complete contract.

	[bookmark: _Toc231466189][bookmark: _Toc231566438][bookmark: _Toc231566557][bookmark: _Toc231566677][bookmark: _Toc231566797][bookmark: _Toc231567060][bookmark: _Toc231567212][bookmark: _Toc233624221]Clause
	[bookmark: _Toc231466190][bookmark: _Toc231566439][bookmark: _Toc231566558][bookmark: _Toc231566678][bookmark: _Toc231566798][bookmark: _Toc231567061][bookmark: _Toc231567213][bookmark: _Toc233624222]Statement
	[bookmark: _Toc231466191][bookmark: _Toc231566440][bookmark: _Toc231566559][bookmark: _Toc231566679][bookmark: _Toc231566799][bookmark: _Toc231567062][bookmark: _Toc231567214][bookmark: _Toc233624223]Data

	10.1
	The Contractor is (Name):
	[bookmark: Text531]     

	
	Address
	[bookmark: Text532]     

	
	Tel No.
	[bookmark: Text533]     

	
	Fax No.
	[bookmark: Text534]     

	11.2(8)
	The direct fee percentage is
	     %

	
	The subcontracted fee percentage is
	[bookmark: Text434]     %

	11.2(14)
	The following matters will be included in the Risk Register
	
[bookmark: Text435]     

	11.2(15)
	The Service Information for the Contractor’s plan is in:
	
[bookmark: Text513]     

	21.1
	The plan identified in the Contract Data is contained in:
	
[bookmark: Text368]     

	24.1
	The key people are:
	

	
	1		Name:
	     

	
			Job:
	     

	
			Responsibilities:
	     

	
			Qualifications:
	[bookmark: Text366]     

	
			Experience:
	[bookmark: Text367]     

	
	2		Name:
	     

	
			Job
	     

	
			Responsibilities:
	     

	
			Qualifications:
	     

	
			Experience:
	     

	
	
	     

	
	
	[bookmark: Text303]CV's (and further key person's data including CVs) are in      .

	A
	Priced contract with price list
	

	11.2(12)
	The price list is in
	[bookmark: Text514]     

	11.2(19)
	The tendered total of the Prices is
	[bookmark: Text369]R     
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	Document reference
	Title
	No of pages

	C2.1
	Pricing assumptions: Option A
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	The price list 
	4







ESKOM HOLDINGS SOC Ltd		CONTRACT NO. _________
PROJECT OR CONTRACT TITLE		



DOCUMENT C2.1	PAGE 2	PRICING DATA	
PART C2 PRICING DATA	PAGE 26 OF 33 	TSC3 OPTION A


C2.1 Pricing assumptions: Option A

[bookmark: _Toc231466193][bookmark: _Toc231566442][bookmark: _Toc231566561][bookmark: _Toc231566681][bookmark: _Toc231566801][bookmark: _Toc231567064][bookmark: _Toc231567216][bookmark: _Toc233624225]How work is priced and assessed for payment
Clause 11 in NEC3 Term Service Contract (TSC3) core clauses and Option A states:

	Identified and defined terms
	11
11.2
	
(12) The Price List is the price list unless later changed in accordance with this contract.


	
	
	(17) The Price for Services Provided to Date is the total of 

the Price for each lump sum item in the Price List which the Contractor has completed and
where a quantity is stated for an item in the Price List, an amount calculated by multiplying the quantity which the Contractor has completed by the rate.


	
	
	(19) The Prices are the amounts stated in the Price column of the Price List. Where a quantity is stated for an item in the Price List, the Price is calculated by multiplying the quantity by the rate.




This confirms that Option A is a priced contract where the Prices are derived from a list of items of service which can be priced as lump sums or as expected quantities of service multiplied by a rate or a mix of both.
[bookmark: _Toc231466194][bookmark: _Toc231566443][bookmark: _Toc231566562][bookmark: _Toc231566682][bookmark: _Toc231566802][bookmark: _Toc231567065][bookmark: _Toc231567217][bookmark: _Toc233624226]Function of the Price List
Clause 54.1 in Option A states: “Information in the Price List is not Service Information”.  This confirms that instructions to do work or how it is to be done are not included in the Price List but in the Service Information.  This is further confirmed by Clause 20.1 which states, “The Contractor Provides the Service in accordance with the Service Information”. Hence the Contractor does not Provide the Service in accordance with the Price List.   The Price List is only a pricing document.  
[bookmark: _Toc231466195][bookmark: _Toc231566444][bookmark: _Toc231566563][bookmark: _Toc231566683][bookmark: _Toc231566803][bookmark: _Toc231567066][bookmark: _Toc231567218][bookmark: _Toc233624227]Link to the Contractor’s plan
Clause 21.4 states “The Contractor provides information which shows how each item description on the Price List relates to the operations on each plan which he submits for acceptance”.  Hence when compiling the price list, the tendering contractor needs to develop his first clause 21.2 plan in such a way that operations shown on it can be priced in the price list and result in a satisfactory cash flow in terms of clause 11.2(17). 
[bookmark: _Toc231466196][bookmark: _Toc231566445][bookmark: _Toc231566564][bookmark: _Toc231566684][bookmark: _Toc231566804][bookmark: _Toc231567067][bookmark: _Toc231567219][bookmark: _Toc233624228]Preparing the price list
Before preparing the price list, both the Employer and tendering contractors should read the TSC3 Guidance Notes pages 14 and 15.  In an Option A contract, either Party may have entered items into the price list either as a process of offer and acceptance (tendering) or by negotiation depending on the nature of the service to be provided.  Alternatively, the Employer, in his Instructions to Tenderers or in a Tender Schedule, may have listed some items that he requires the Contractor to include in the price list to be prepared and priced by him. 

It is assumed that in preparing or finalising the price list the Contractor:

· Has taken account of the guidance given in the TSC3 Guidance Notes relevant to Option A;
· Understands the function of the Price List and how work is priced and paid for;
· Is aware of the need to link operations shown in his plan to items shown in the Price List;
· Has listed and priced items in the price list which are inclusive of everything necessary and incidental to Providing the Service in accordance with the Service Information, as it was at the time of tender, as well as correct any Defects not caused by an Employer’s risk;
· Has priced work he decides not to show as a separate item within the Prices or rates of other listed items in order to fulfil the obligation to complete the service for the tendered total of the Prices. 
· Understands there is no adjustment to items priced as lump sums if the amount, or quantity, of work within that item later turns out to be different to that which the Contractor estimated at time of tender. The only basis for a change to the (lump sum) Prices is as a result of a compensation event. 

[bookmark: _Toc231466197][bookmark: _Toc231566446][bookmark: _Toc231566565][bookmark: _Toc231566685][bookmark: _Toc231566805][bookmark: _Toc231567068][bookmark: _Toc231567220][bookmark: _Toc233624229]Format of the price list
(From the example given in an Appendix within the TSC3 Guidance Notes)

Entries in the first four columns in the price list in section C2.2 are made either by the Employer or the tendering contractor. 

If the Contractor is to be paid an amount for the item which is not adjusted if the quantity of work in the item changes, the tendering contractor enters the amount in the Price column only, the Unit, Expected Quantity and Rate columns being left blank.

If the Contractor is to be paid an amount for an item of work which is the rate for the work multiplied by the quantity completed, the tendering contractor enters the rate which is then multiplied by the Expected Quantity to produce the Price, which is also entered.

If the Contractor is to be paid a Price for an item proportional to the length of time for which a service is provided, a unit of time is stated in the Unit column and the expected length of time (as a quantity of the stated units of time) is stated in the Expected Quantity column.
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C2.2 the price list


	Item nr
	Description
	Unit
	Expected Quantity per Year
	Rate
	Price

	1
	Preliminaries and General
	
	
	
	

	1.1
	Site establishment (once-off)
	each
	1
	
	

	1.2
	De-establishment (once-off)
	each
	1
	
	

	1.3
	Health and Safety File documentation, staff medicals &  PPE
	annual
	1
	
	

	1.4
	Transport (Fixed monthly operational transport)
	month
	12
	
	

	1.5
	Accommodation
	month
	12
	
	

	1.6
	Safety Officer Fee (Part-time, twice a week for the duration of the contract)
	month
	12
	
	

	1.7
	Site supervision + Pest Control Officer Fee
	month
	12
	
	

	2
	Maintain Lawns and Gardens
Short lawn maintenance (30–50mm), lawn mowing, edging, trimming, pruning, herbicide application and weed control. Frequency shifts seasonally: Bi-weekly during the growing season (September to April) and Monthly during the winter/dry season (May to August).

	2.1
	Surface Building lawns – 2390 m² (Bi‑weekly (growing season) / Monthly (dry season)
	service cycle
	20
	
	

	2.2
	Visitor Centre lawns – 8 442 m² (Bi‑weekly (growing season) / Monthly (dry season)
	service cycle
	20
	
	

	2.3
	Stores & Park homes – 3 167 m² (Bi‑weekly (growing season) / Monthly (dry season)
	service cycle
	20
	
	

	2.4
	Water Treatment Plant lawns – 1 133 m² (Bi‑weekly (growing season) / Monthly (dry season)
	service cycle
	20
	
	

	2.5
	Jagersrust pavements – 4 500 m² (Bi‑weekly (growing season) / Monthly (dry season)
	service cycle
	20
	
	

	2.6
	Single quarters– 5 755 m²  (Bi‑weekly (growing season) / Monthly (dry season)
	service cycle
	20
	
	

	2.7
	Post office & lodge – 17 608 m² (Bi‑weekly (growing season) / Monthly (dry season)
	service cycle
	20
	
	

	2.8
	Annual provision of mulch and fertilisers
	service cycle
	1
	
	

	3
	Road Verges, Access Roads, Servitudes and Tunnel Entrances
Grass cutting on both sides of road verges, herbicide application, removal of encroaching vegetation and alien plants, and sweeping/cleaning/blowing of road surfaces/paved areas. Cleaning of storm water drains.

	3.1
	Entrance Road from R74 to T-junction (Road A) - 3.3 km
	month
	12
	
	

	3.2
	Main access road to Surface Building (Road B) - 6 km
	month
	12
	
	

	3.3
	T-Junction to Jagersrust (Road C) - 1.5 km
	month
	12
	
	

	3.4
	Tunnel Entrances (Tunnel 1,2,3) including Vegetation Clearing (Monthly/As and when required) - 225 m²
	month
	12
	
	

	3.5
	Stores access road (Road D) - 1 km
	month
	12
	
	

	3.6
	Headrace road (Monthly/As and when required) - 0.5 km
	month
	12
	
	

	3.7
	Infrastructure and dam roads (SH, MAT, T2&3, KB, Link yard, JWR) (Monthly/As and when required) – 1.3 km
	month
	12
	
	

	4
	Fenced and Restricted Operational Areas (grass cutting and vegetation management)
Grass cutting, alien vegetation eradication, and herbicide maintenance twice a month to keep stone-chipped, paved, and fenced perimeters permanently free of vegetation.

	4.1
	1m outside the perimeter fence: Headrace 451 m², surge shaft 590 m², Jagersrust Water Reservoir 148 m², STP 59 m² & Scrap Storage Area 69 m² fence Perimeter (Monthly/ As and when required) 
	month
	12
	
	

	4.2
	Headrace (Entire footprint) (Monthly/ As and when required) – 8311 m²
	month
	12
	
	

	4.3
	Surge Shaft (Entire footprint) (Monthly/ As and when required) – 16 505 m²
	month
	12
	
	

	4.4
	Jagersrust Water Reservoir (Yard) (Monthly/ As and when required) – 1004 m²
	month
	12
	
	

	4.5
	1m outside the perimeter fence (both): Jagersrust Village Palisade Fence (Monthly/ As and when required) – 1102 m²
	month
	12
	
	

	5
	Stone chipped areas
Grass cutting, alien vegetation eradication, and herbicide maintenance twice a month to keep stone-chipped, paved areas permanently free of vegetation.

	5.1
	Headrace (Inner fenced area) (Monthly/ As and when required) – 5077 m²
	month
	12
	
	

	5.2
	Surge Shaft (Inner fenced area) (Monthly/ As and when required) – 6318 m²
	month
	12
	
	

	5.3
	Scrap Storage Area (Yard) (Monthly/ As and when required) – 233 m²
	month
	12
	
	

	5.4
	STP (Yard) (Monthly/ As and when required) – 160 m²
	month
	12
	
	

	6
	Critical infrastructure
Critical infrastructure clearance zones maintained free of tall grass, shrubs, and weeds for infrastructure protection and fire risk mitigation.

	6.1
	2m wide Walkway/Path leading from the Surface Building/Station to the Fire Reservoir/Diesel Generator Deluge Dam and 5m radius around the Reservoir - 541 m²
	month
	12
	
	

	6.2
	Pole Mounted Transformers – 150 m²
	month
	12
	
	

	6.3
	Kilburn Dam TV Repeater – 681 m²
	month
	12
	
	

	6.4
	Air Intake Structures – 110 m²
	month
	12
	
	

	6.5
	Station Air Intake – 100 m²
	month
	12
	
	

	6.6
	Lift Shaft Ventilation – 100 m²
	month
	12
	
	

	6.7
	Breaker & Link Yard – 90 m²
	month
	12
	
	

	6.8
	Main Water Supply Valve – 100 m²
	month
	12
	
	

	6.9
	Boreholes & access paths - 600 m²
	month
	12
	
	

	6.10
	Temporary Supply Area – 200 m²
	month
	12
	
	

	6.11
	Access Paths to Springs – 200 m²
	month
	12
	
	

	7
	Monthly and Weekly Routine Work
	
	
	
	

	7.1
	Water and maintain indoor & outdoor plants (once a week)
	week
	52
	
	

	7.2
	Remove refuse from bins (Plant, stores, VC, MAT, parking) (twice a week)
	week
	104
	
	

	7.3
	Remove general waste and garden refuse at Jagersrust twice a week (only outside Eskom residents) 
	week
	104
	
	

	7.4
	General cleaning and maintenance of roads, walkways, paved, parking areas (weekly)
	week
	52
	
	

	7.5
	Record and report water meter readings for all applicable facilities (monthly)
	month
	12
	
	

	8
	Additional / Ad‑Hoc Services (As & When required)
	
	
	
	

	8.1
	Irrigation services (all landscaped areas)
	service cycle
	12
	
	

	8.2
	Unblock stormwater drains (additional requirements during rainy seasons)
	service cycle
	4
	
	

	8.3
	Establish new flower beds per 25m² (soil prep, planting) 
	service cycle
	4
	
	

	8.4
	Supply & plant indigenous trees (3 per year)
	each
	3
	
	

	8.5
	Excavate trenches for maintenance works - 1 km, depth 3m, width 1m  
	service cycle
	6
	
	

	8.6
	Grass cutting, tree pruning, mowing and weeds removal of vacant house yards
	each
	12
	
	

	
	
	
	
	
	



	The total of the Prices
	

	The total of the Prices for 5 Years
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1. [bookmark: _Toc137798038][bookmark: _Toc229128241][bookmark: _Toc232953634][bookmark: _Toc516836502][bookmark: _Toc231566449][bookmark: _Toc231566568][bookmark: _Toc233624232]
Description of the service

1.1. [bookmark: _Toc137798039][bookmark: _Toc229128242][bookmark: _Toc232953635][bookmark: _Toc516836503][bookmark: _Toc231566450][bookmark: _Toc231566569][bookmark: _Toc233624233]Executive overview 

Provision of gardening services at Drakensberg Pumped Storage Scheme, for the period of 5 years. The services include lawn maintenance (routine and seasonal care), landscape plant maintenance (trees, shrubs, ground cover), other general maintenance and tree felling. 

1.2. [bookmark: _Toc137798056][bookmark: _Toc229128259][bookmark: _Toc232953636][bookmark: _Toc516836504][bookmark: _Toc231566451][bookmark: _Toc231566570][bookmark: _Toc233624234]Employer’s requirements for the service

The Contractor provides labour including supervision, tools - including special tools, equipment – including special equipment, Plant and Material, consumables necessary to carry out the service.

1.2.1. [bookmark: _Toc233624235]Maintenance of Lawns and Gardens

These areas require frequent mowing, edging, trimming, weeding, pruning, mulching, flower bed maintenance, pest monitoring and annual application of fertilizer. Grass shall be maintained short at all times. Weeding and removal of alien invasive plants are mandatory in all areas. The supplier shall identify areas for grass re-establishment; on approval, these areas shall be revegetated with the approved lawn seed. Frequency will be bi-weekly for the growing season (September to April) and dry season (May to August) resulting in 20 service cycles per year for the duration of the contract.

1.2.1.1. Mowing
Frequency: Weekly during growing season; monthly during dry season
· Paper, trash, branches, and flowers not associated with the specific area, including all other debris, will be collected prior to each mowing. 
· Contractor will mow turf areas as needed according to seasonal growth/on the following schedule: as per the attached list above. 
· Contractor will be expected to adjust the mowing height as appropriate and, if necessary, for different sections of the site. Lawn areas must be maintained at a uniform height of approximately 30–50 mm after mowing, unless otherwise instructed by the Employer. 
· During periods of excessive rain and tall grass growth, the mower cut height may be raised. 
· Brush cutters may be used around structures, poles, edges, barriers, fences, trees, dirt roads, unpaved footpaths, dense vegetation, or where reel/rotary mowers cannot be used. 
· All mowing shall be carried out using a reel or rotary mower. 
· Mower blades shall be kept sharp at all times to ensure a quality cut and to prevent tearing of grass blades. 
· Appropriate mowing equipment and patterns (including alternating directions where possible) shall be used to promote the recycling of clippings and maintain a neat appearance. 
· Grass clippings shall be left on the lawn provided that no visible clumps remain on the surface 36 hours after mowing. Where clumps are present, the Contractor shall redistribute them using mechanical blowers or remove them. In cases of fungal disease outbreaks, all clippings shall be collected and removed until the disease is no longer evident. 
· Areas with coping adjacent to grass shall be maintained with due care using brush cutters or edge cutters where required. 
· No coping shall be damaged or removed during turf maintenance. Mowers shall not be operated over coping. 

1.2.1.2. [bookmark: _Toc231566571]Edging and Trimming 
Frequency: Weekly, aligned with mowing schedule.

· Grass adjacent to fixed objects shall be trimmed to the same height as the surrounding turf. Trimming shall be undertaken in a manner that prevents scalping of turf areas. 
· The Contractor shall edge all tree rings and plant beds. In addition, all buildings, sidewalks, fences, driveways, parking areas, and any other surfaced areas bordered by grass shall be edged at least every alternate mowing cycle. 
· When trimming or cutting near the Employer’s or staff property (including vehicles), the Contractor shall ensure that the rotation of the trimmer directs debris away from such property. Where necessary, a suitable barrier (e.g., netting or shade cloth) shall be used to prevent objects such as stones, sticks, or debris from being projected, thereby minimising the risk of damage. 
· Isolated trees and shrubs located within lawn areas shall have mulched rings around their bases to prevent bark damage from mowing equipment and to reduce competition from grass. The establishment and ongoing maintenance of these mulched areas shall be for the Contractor’s account. 
· The Contractor shall remove all grass clippings from sidewalks, curbs, roadways, markers, and other hard surfaces immediately after mowing and/or edging. Under no circumstances shall clippings be swept, blown, or otherwise disposed of into stormwater drains or sewer systems. 
· The Contractor shall ensure that grass clippings do not accumulate in corners or confined areas around buildings or infrastructure, as this may lead to unsightly build-up of dead organic material over time. 
· The use of herbicides as a substitute for proper edging and trimming is strictly prohibited, particularly adjacent to buildings, walkways, drainage features (including V-drains), and other infrastructure. 

1.2.1.3. Pruning
· Any growth of branches, etc., overhanging roofs of buildings, walls, fences, carports, etc., which can cause damage or the depositing of leaves, etc. in storm water gutters or on roofs is to be regularly trimmed. Any growth of plants that can damage fences or compromise security, or obstruct vision, is to be removed.
· Pruning should also be done to remove dead or diseased branches, reduce foliage density or crossing branches, to improve the beauty of the shrub or trees through selective removal of a few branches
· Shrubs will be pruned with hand shears as needed to provide an informal shape, fullness and blooms.
· The Contractor must remove all litter from the surrounding area.

1.2.1.4. [bookmark: _Toc231566572]Aeration 
Frequency: Once or twice annually (spring and/or fall).
· Turf grass areas in regions of clay and highly compacted soils require regular aeration. Aeration should be accomplished in the early spring. 

1.2.1.5. Pest & Disease Control

Frequency: Monthly inspections; treatments as required

· The Contractor will inspect lawn areas each visit for indications of pest problems and advise the Employer’s representative of such problems. 
· The Contractor will keep records of pests identified and treatment(s) rendered for control. 
1.2.1.6. [bookmark: _Toc231566573]Herbicide

Herbicide to be applied in an environmentally friendly manner to prevent the sterilization of soil and pollution of a water resource. Specific applications include cutting of invasive alien plants, treatment of all paved, concrete, stone-chipped and tarred surfaces and V trenches. 
		
1.2.1.7. Mulching 

All mulched areas are replenished once a year during the winter months. 
· Mulch should be maintained at a depth of not less than 100 mm and 200 mm.
· Mulch will not be placed against the trunks of plants.
· Mulch will not be allowed to cover valve boxes, meters etc.
· All curb, roadway and bed edges are trenched to help contain the applied mulch. The Contractor is required to define all edges and taper or roll away the mulch from the edges. 
· The Contractor is responsible for remixing mulch in areas that are starting to show mould or rot and to ensure that mulch or other landscape bed materials are not mixing or creeping into turf areas. 

1.2.1.8. Paved and stone-chipped areas

All stone chipped, paved paths and roads within these areas must be kept free of any vegetation, weeds and swept to prevent soil and litter build up. 







Table 1: Maintain Lawns and Gardens

	Item 
	Area Description 
	Area (m²) 
	Frequency 

	3.1.1 
	Surface building 
	2390 m² 
	Bi‑weekly (growing season) / Monthly (winter) 

	3.1.2 
	Visitor Centre 
	8442 m² 
	Bi‑weekly (growing season) / Monthly (winter) 

	3.1.3 
	Stores and Park homes 
	3167 m² 
	Bi‑weekly (growing season) / Monthly (winter) 

	3.1.4 
	Jagersrust Water Plant 
	1133 m² 
	Bi‑weekly (growing season) / Monthly (winter) 

	3.1.5 
	Pavements – Jagersrust (1.5 km) 
	4500 m² 
	Bi‑weekly (growing season) / Monthly (winter) 

	3.1.8 
	Single Quarters 
	5755 m² 
	Bi‑weekly (growing season) / Monthly (winter) 

	3.1.9 
	Post Office, Club House and Sunset Lodge 
	17 608 m² 
	Bi‑weekly (growing season) / Monthly (winter) 

	3.1.10 
	Vacant Eskom Houses 
	
	As required



1.2.2. [bookmark: _Toc233624236]Road Verges, Access Roads, Servitudes and Tunnel Entrances
Vegetation management shall be undertaken along all DPSS roads, access routes, servitudes and tunnel entrances to maintain visibility, accessibility, infrastructure protection, and fire prevention. Cutting includes signs, barriers and culverts.

1.2.2.1. Grass Cutting and Verge Maintenance
· The Contractor shall cut grass on both sides of road verges to a minimum width of 3 m from the road edge, unless otherwise specified.
· Cutting shall be undertaken using brush cutters, ride-on mowers or appropriate equipment, depending on terrain.
· Road verges must be maintained at a maximum grass height of 100 mm unless otherwise instructed by the Employer.
· Care must be taken to avoid scalping, soil disturbance, and erosion, especially in sensitive areas.
· Cutting of grass, bushes and removal of trees, including roots where necessary, within a distance of 5 metres to the left, 5 metres to the right, and 5 metres above each tunnel entrance, measured from the outer face of the tunnel portal, for a total of three (3) tunnel entrances.
· Remove all grass cuttings, stones, litter and debris from the road surface immediately after cutting.
· Prevent any material from entering stormwater systems.
· Ensure vegetation around road signs, barriers, guardrails, fences and other infrastructure is kept clear at all times.
· Sweeping shall be conducted regularly to prevent sediment accumulation.
· Vegetation in V‑trenches, stormwater drains and channels shall be removed.
· All collected material shall be transported to designated disposal areas.
· Cleaning of the road surfaces to remove small stones, sand and debris to prolong the surface of the road due to the heavy traffic experienced on the roads. The service includes all internal roads and all hard surfaces surrounding the buildings. Cleaning can be done through the use of a combination of brooms and mechanical blowers.

1.2.2.2. Tree Pruning
· Prune or cut back trees and shrubs encroaching onto roads or obstructing visibility, signage, or infrastructure.
· Remove any dead, damaged, or vegetation that may pose a risk to road users or infrastructure.
· Ensure adequate clearance for vehicles, including heavy-duty and emergency vehicles.

1.2.2.3. Invasive Alien Plant Control
· Remove and control invasive alien plant species within road verges and servitudes (up to 5 m or fence line, where applicable).
· Control methods must align with NEM:BA requirements and use only approved, environmentally appropriate herbicides.
· Follow an integrated approach (mechanical and chemical where required) and prevent regrowth through follow-up treatments.



Table 2: Access Roads and tunnel entrances
	Item 
	Area Description 
	Estimated area (km/m2) 
	Frequency 

	3.2.1 
	Entrance Road from R74 to T-junction (Road A) 
	3.3 km 
	Monthly 

	3.2.2 
	Main access road to Surface Building (Road B) 
	6 km 
	Monthly 

	3.2.3 
	T-Junction to Jagersrust (Road C) 
	1.5 km 
	Monthly 

	3.2.4 
	Stores access road (Road D) 
	1 km 
	Monthly 

	3.2.5 
	Headrace access road 
	0.5 km 
	Monthly 

	3.2.6 
	Access roads to dams and station infrastructure (SH, MAT, T2&3, KB, Link yard, JWR) 
	1.3 km 
	Monthly 

	3.2.7 
	Vegetation clearing at tunnel entrances (Tunnel 1, 2 & 3) 
	225 m2 
	Monthly 



1.2.3. [bookmark: _Toc233624237]Fenced and Restricted Operational Areas
Vegetation shall be controlled inside and outside all operational and security fences to ensure security visibility, infrastructure protection and fire prevention. The following requirements apply to the five fenced areas (Headrace, Surge Shaft, Jagersrust Water Reservoir, Sewage Plant and Scrap Yard). Frequency shall be monthly, increasing to bi‑weekly during peak growth periods where required.

1.2.3.1. Surge Shaft and Headrace (Driekloof) Security Fence area 
· Complete the area between the inner and outer fences, and 1m outside the perimeter of the outer fence 
· Cut grass and control alien vegetation within the surge and headrace fenced area 
· The inner fenced areas (stone chipped) shall be maintained free of all vegetation at all times. 
· All stone-chipped, paved paths and tarred areas must be kept free of any vegetation, weeds through mechanical and approved chemical means and swept to prevent soil and litter build-up. 
· Remove weeds/grass growing on the road surfaces and perform weed control by using environmentally appropriate herbicides. 
· Removal of stones and debris on the road surface once the grass is cut. 
· Clean and cut grass on culverts. 
· Remove all vegetation in stormwater channels next to the road and perform weed control by using environmentally appropriate herbicides. 
· Clear vegetation 1 meters on the outside of the surge and headrace fence to allow for security to perform their walkabout. 

1.2.3.2. Sewage Treatment Plant and Scrap Storage Area 
· Complete yard, including 1m around the outside perimeter of the fence. 
· Remove weeds/grass growing on the sewage water treatment plant and scrap storage area and perform weed control by using environmentally appropriate herbicides. 
· Removal of stones and debris on road surface once the grass is cut. 
· Clean and cut grass on culverts. 
· Remove all vegetation in stormwater channels next to the road and perform weed control by using environmentally appropriate herbicides. 
· Cut grass and control alien vegetation within the Sewage Treatment Plant and Scrap Storage fenced area 
· Clear vegetation 1 meter on the outside of the Sewage Treatment Plant and Scrap Storage fence 
· Removal of all vegetations growing in the fence area, and perform invasive alien plant control by using environmentally appropriate herbicides 

1.2.3.3. Jagersrust Palisade fence 
· Clean both sides of the concrete palisade fence along the perimeter. 
· Cut grass and remove trees and shrubs 1 meter from both sides of the concrete palisade fence. 
· Remove weeds/grass growing on the fence and perform weed control by using environmentally appropriate herbicides




Table 3: Fenced and Restricted Operational Areas
	Item 
	Area Description 
	Area (m²) 
	Frequency 

	Headrace 

	3.2.1.1 
	Headrace (entire footprint inside the inner fence) 
	8311 m² 
	Monthly 

	3.2.1.2 
	Headrace (Inner fenced area) 
	5077 m² 
	Monthly 

	3.2.1.3 
	Headrace (1m outside the perimeter of the outer fence) 
	451 m² 
	Monthly 

	Surge Shaft 

	3.2.2.1 
	Surge Shaft (entire footprint inside the inner fence) 
	16505 m² 
	Monthly 

	3.2.2.2 
	Surge Shaft (Inner fenced area) 
	6318 m² 
	Monthly 

	3.2.2.3 
	Surge Shaft (1m outside the perimeter of the outer fence) 
	590 m² 
	Monthly 

	Jagersrust Water Reservoir 

	3.2.3.1 
	Jagersrust Water Reservoir (entire yard) 
	1004 m² 
	Monthly 

	3.2.3.2 
	Jagersrust Water Reservoir (1m outside the perimeter fence) 
	148 m² 
	Monthly 

	Sewage Plant 

	3.2.4.1 
	Sewage Plant (entire yard) 
	160 m² 
	Monthly 

	3.2.4.2 
	Sewage Plant (1m outside the perimeter fence) 
	59 m² 
	Monthly 

	3.2.5.1 
	Scrap Storage Area (entire yard) 
	233 m² 
	Monthly 

	3.2.5.2 
	Scrap Storage Area (1m outside the perimeter fence) 
	69 m² 
	Monthly 

	3.2.5.3 
	Jagersrust village concrete palisade fence 
	1102 m2 
	Monthly 



1.2.4. [bookmark: _Toc233624238]Station Operational Equipment, Infrastructure, and Monitoring & Testing Areas 

Critical infrastructure clearance zones shall be maintained permanently free of tall grass, shrubs and trees to ensure operational safety, access for maintenance, and fire risk mitigation. Vegetation shall be kept low, and access paths clearly defined and maintained. 

Table 4: Station Operational Equipment, Infrastructure, and Monitoring & Testing Areas
	Item 
	Area Description 
	Area (m²) 
	Frequency 

	3.4.1 
	2m wide walkway/path leading from the Surface building/Station to the Fire Reservoir/Diesel generator deluge dam and 5m radius around the Reservoir 
	541 m2 
	Monthly 

	3.4.2 
	Pole mounted transformers 
	150 m2 
	Monthly 

	3.4.3 
	10m radius around the Kilburn dam-level Building TV – Repeater 
	681 m2 
	Monthly 

	3.4.4 
	Air intake / ventilation structures 
	110 m2 
	Monthly 

	3.4.5 
	5m radius around the Station Air Intake Structure 
	100 m2 
	Monthly 

	3.4.6 
	5m radius around the Lift shaft ventilation structure 
	100 m2 
	Monthly 

	3.4.7 
	5m radius around the Breaker and Link Yard 
	90 m2 
	Monthly 

	3.4.8 
	1m radius around the Drakensville main water supply valve. Valve - Jagersrust Farm. 
	100 m2 
	Monthly 

	3.4.9 
	5m radius around all boreholes and a 2m wide path leading to them 
	600 m2 
	Monthly 

	3.4.10 
	2m wide walkway/path leading from the Temp supply and 5m radius around the Temp supply 
	200 m2 
	Monthly 

	3.4.11 
	Access foot paths to Springs/Testing Area x 2 
	200 m2 
	Monthly 



1.2.5. [bookmark: _Toc233624239]Herbicide Application and Alien and Invasive Plant Management 
· Specific applications shall include, but not be limited to, the following areas: all paved concrete, stone-chipped, and tarred surfaces; all tarred road verges; the Headrace; Surge Shaft; Jagersrust Water Treatment Plant; Jagersrust Water Reservoir; areas surrounding boreholes; and the Kilburn building. 
· Only registered, environmentally friendly herbicides approved by Eskom shall be used. 
· Removal of alien invasive plants is mandatory in all areas covered by this scope. 
· Herbicide application as required must be applied at all times under the direct supervision of a registered Pest Control Operator (PCO), in accordance with the Fertilizers, Farm Feeds, Agricultural Remedies and Stock Remedies Act, 1947 (Act No. 36 of 1947), and all applicable Eskom standards and legal requirements. 
· Herbicide use supports, but does not replace, mechanical and manual control. 
· Herbicides are to be applied in accordance with the manufacturer’s specifications and are to be carried out by a competent person wearing the correct protective clothing. 
· Alien and invasive plant species shall be identified, removed and controlled across all work areas. Common species found in DPSS include, but are not limited to, Bugweed (Solanum mauritianum), Bramble (Rubus spp.), Tick berry (Lantana camara) 
· Removal shall occur prior to flowering or seeding, with follow‑up control mandatory. 
· The Contractor shall be in possession of the relevant Hazchem certificates and is to ensure that the handling of all hazardous chemical substances, including fertilizers, is strictly in accordance with the Regulation for Hazardous Chemical substances framed under the OSH Act No. 85 of 1993. All Hazchem data sheets are to be forwarded for all chemicals used. 
· All empty herbicides and fertiliser containers are to be immediately disposed of off-site in accordance with the relevant laws, by-laws, and regulations 



1.2.6. [bookmark: _Toc231566574][bookmark: _Toc233624240]Other General Maintenance 

1.2.6.1.  Weekly Routine Work

[bookmark: _Toc231566575]The Contractor shall perform the following routine activities on a weekly basis to maintain acceptable environmental, operational, and aesthetic standards: 
· Maintain all flower beds at the Visitor Centre, Guest Houses, and Kilburn Heights, including weeding, trimming, soil conditioning, and general upkeep. 
· Sweep all paved areas surrounding the Surface Building, ensuring removal of dirt, mud, litter, and any foreign debris. 
· Ensure that all sand beds at the Drakensberg Surface Sewage Treatment Plant are kept free of weeds at all times. 
· Sweep and clean the cemented area at Tunnel One, removing all debris, loose rocks, and accumulated mud. 
· Water and clean all indoor and outdoor plants located within the Surface Building, OPS Control Room, and external paved areas near turnstiles and office entrances. Care shall be taken to prevent overwatering. 
· Remove refuse from domestic waste bins at least twice per week from the Stores, Visitor Centre, Main Access Tunnel, and all parking areas. Waste shall be transported to designated disposal areas. 
· Collect and remove litter from all Eskom-managed areas, including roads, parking areas, and Jagersrust Village, to maintain a clean and safe environment. 

1.2.6.2. [bookmark: _Toc231566576]Monthly Routine Work 
[bookmark: _Toc231566577]The Contractor shall undertake the following activities on a monthly basis to ensure the sustained upkeep of landscaped areas and operational environments:

· Manually remove all weeds from landscape beds (including barked, stone-covered, and flower beds), as well as from curbs, coping edges, sidewalks, parking areas, fence lines, retaining walls, property boundaries, and any other areas where weeds occur. This shall include the ongoing maintenance and controlled watering of all office flowers and landscaped features. 
· Remove all litter and foreign material from planting beds and other high-visibility areas, including walkways, roads, and parking areas, to maintain a clean and presentable environment. 
· Ensure that all turf areas and planting beds (including shrubbery and landscaped zones) are cleared of leaves, weeds, litter, and any other debris during each scheduled service visit. 
· Record and report water meter readings for all applicable facilities, including Jagersrust Village, the farm, and associated resorts, in accordance with site reporting requirements. 
	
1.2.6.3. Additional and Ad-Hoc Services 
The Contractor shall provide the following additional services on an as-and-when required basis, as directed by the Employer: 
· Provide irrigation services for existing and future landscaped areas, including bedding plants, trees, and office flowers. This includes irrigation required for special events such as Arbor Day. Irrigation shall be conducted responsibly to promote plant health while avoiding overwatering. 
· Unblock and clean all stormwater, and seepage drainage systems at Jagersrust residences, Stores, Visitor Centre, and Station facilities to ensure proper functionality and prevent blockages. 
· Establish new flower beds and garden features as instructed by the Employer from time to time. This shall include: 
· Removal of existing grass and unwanted vegetation 
· Soil preparation and conditioning 
· Application of fertiliser and herbicide 
· Planting in accordance with Employer specifications The Employer shall provide the required flora and fertiliser, while the Contractor shall be responsible for planting, establishment, and ongoing irrigation. 
· Supply three (3) indigenous trees annually for Arbor Day celebrations and support their planting and establishment where required. 
· Cut and trim tree branches that overhang or obstruct roads, buildings, and infrastructure within Jagersrust and along access routes to the Pumped Storage Scheme to ensure safety and accessibility. 
· Excavate trenches as required to support maintenance, drainage, or operational activities. 
· Sweep all roads and remove stones, debris, and obstructions to maintain safe and usable access routes. 
· Collect, load, and transport all garden refuse to designated biodegradable waste disposal areas in accordance with site requirements. 
· Clean and remove sediment, vegetation, and debris from earth-lined and concrete drainage channels along roads. 
· Inspect and clean all road culverts to ensure effective stormwater flow and prevent blockages. 

1.2.7. [bookmark: _Toc233624241]Staffing, Equipment, Storage and Waste Management 
The Contractor shall ensure that adequate resources, systems, and controls are in place to effectively deliver the required services in a safe, compliant, and environmentally responsible manner. 
1.2.7.1. Staffing and Resources 
· The Contractor shall provide all labour, supervision, tools, equipment, plant, and consumables necessary for the execution of the services. 
· All personnel shall undergo DPSS site-specific Safety, Health, and Environmental (SHE) induction, as well as security screening and medical clearance, prior to commencement of work. 
· A full complement of appropriately trained and competent staff shall be maintained at all times to ensure continuous service delivery. 
· Relief and replacement personnel shall meet the same induction, medical, and competency requirements as permanent staff. 

1.2.7.2. Equipment and Operations 
· All vehicles, plant, and equipment shall be properly maintained and remain in good working condition at all times. 
· Servicing, repairs, and maintenance of vehicles and equipment shall be conducted off-site at approved facilities. 
· The Contractor shall ensure that sufficient backup equipment is readily available to maintain uninterrupted service delivery in the event of breakdowns or failures. 

1.2.7.3. Storage and Materials Handling 
· No bulk storage of fertilisers, compost, or other materials shall be permitted on site unless prior written approval has been obtained from the Employer. 
· All materials brought onto site shall be managed in a manner that prevents environmental contamination, safety risks, or operational disruption. 


1.2.7.4. Waste Management 
· All garden refuse and domestic waste generated from the execution of the services shall be collected and disposed of at a licensed and registered waste disposal facility, unless otherwise approved by the Employer.
· No temporary or satellite waste storage areas shall be established on site without prior approval. 
· Waste shall be handled, transported, and disposed of in accordance with applicable environmental legislation and Eskom requirements. 
· The Contractor shall submit proof of safe and compliant disposal (e.g., waste disposal certificates or weighbridge slips) to the Service Manager as required. 

1.2.8. [bookmark: _Toc233624242]Minimum Resources 
	No.
	Plant
	Description

	1
	5 x Brush cutters
	For grass cutting on slopes, road verges, fence lines, and restricted areas

	2
	3 x Lawn mowers
	For mowing grass around offices, residential and landscaped areas

	3
	2 x Chainsaws
	For cutting tree branches, bush clearing, and invasive plant removal

	4
	3 x Pruning shears/loppers
	For pruning shrubs, hedges and branches

	5
	4 x Rakes
	For collection of grass cuttings, leaves and debris

	6
	4 x Garden forks
	For soil turning and mulch handling

	7
	4 x Spades
	For digging, trenching and planting

	8
	2 x Wheelbarrows
	For transporting soil, mulch and garden waste

	9
	4 x Mechanical blowers
	For cleaning roads and paved areas

	10
	4 x Brooms
	For sweeping paved areas and walkways

	11
	2 x Hose pipes (50m)
	For watering gardens and cleaning

	12
	3 x Knapsack sprayers (15–20 litre)
	For herbicide and pesticide application

	15
	1 x Light delivery vehicle
	For transporting staff and equipment

	16
	1 x Trailer
	For transporting garden refuse

	17
	2 x Drip tray
	For preventing oil, fuel, and chemical spills during refuelling and maintenance

	18
	2 x Spot-spray applicators / spray bottles
	Targeted herbicide treatment

	19
	2 x Hand saws and bow saws
	Manual cutting of thicker stems






1.3. [bookmark: _Toc137798041][bookmark: _Toc229128244][bookmark: _Toc232953637][bookmark: _Toc516836505][bookmark: _Toc231566452][bookmark: _Toc231566578][bookmark: _Toc233624243]Interpretation and terminology

	Definition 
	Explanation 

	Site / Power Station 
	The operational footprint and associated properties of Drakensberg Pumped Storage Scheme, including fenced areas, servitudes, access roads, laydown areas, buffer zones, and adjacent Eskom-owned land. 

	Vegetation Management 
	A coordinated set of activities to maintain, control, or remove vegetation to meet safety, compliance, ecological, and operational objectives, including garden services, invasive species control, and fire risk mitigation. 

	Garden Services / Grounds Maintenance 
	Routine maintenance of landscaped and common areas, including lawn cutting, edging, pruning, hedge trimming, litter removal, sweeping, rinsing/power-washing of hard surfaces where specified, irrigation system checks, and compost/mulch application as required. 

	Alien Plant 
	A plant species that is not indigenous to South Africa or the local bioregion where the site is situated. 

	Invasive Alien Plant 
	An alien plant that spreads aggressively and causes environmental, economic, or social harm, requiring control or eradication in terms of applicable legislation and site procedures. 

	Invasive Categories (1a, 1b, 2, 3) 
	Administrative categories used to describe management obligations for invasive alien species. Category 1a: eradicate; 1b: control and prevent spread; 2: regulated restricted to permit conditions; 3: listed for control in specific areas/conditions. 

	Indigenous / Native Species 
	Plant species that naturally occur within South Africa and within the local bioregion of the site. 

	Fence Line Clearing 
	Vegetation removal and trimming along perimeter and internal fences to maintain access, visibility, security integrity, and firebreak continuity. 

	Mechanical Control 
	Physical removal or reduction of vegetation using manual labour or equipment (e.g., brush cutters, chainsaws, mowers, mulchers, hand-pulling, grubbing). 

	Chemical Control 
	Use of approved herbicides to control vegetation, including foliar, cut-stump, basal bark, or soil-applied treatments, in accordance with label instructions and legal requirements. 

	Variation
	Any change to scope, method, or frequency approved by the Client in writing, including adjustments due to operational constraints, weather, or ecological sensitivities.

	Method Statement
	Contractor’s written procedure describing how specific tasks will be executed safely and compliantly, including equipment, sequence of work, PPE, environmental controls, waste handling, and emergency response.

	Herbicide 
	A chemical substance used to inhibit or kill unwanted vegetation, applied in accordance with product labels, legal requirements, and site procedures. 

	Waste 
	Any material arising from vegetation activities requiring collection and proper disposal or reuse (e.g., green waste, invasive biomass, packaging, chemical containers), managed per the waste hierarchy and site procedures. 

	Edge / Verge 
	The linear strip adjacent to roads, paths, or fence lines 




The following abbreviations are used in this Service Information:

	Abbreviation
	Meaning given to the abbreviation

	SHEQ
	Safety, Health, Environment, and Quality

	PPE
	Personal Protective Equipment

	FPA
	Fire Protection Association

	QA
	Quality Assurance

	HIRA
	Hazard Identification and Risk Assessment

	OHSA
	Occupational Health and Safety Act

	NEMA
	National Environmental Management Act

	ISO
	International Organization for Standardization

	NEMBA
	National Environmental Management: Biodiversity Act

	QCP
	Quality Control Plan





2. [bookmark: _Toc137798042][bookmark: _Toc229128245][bookmark: _Toc232953638][bookmark: _Toc516836506][bookmark: _Toc231566453][bookmark: _Toc231566579][bookmark: _Toc233624244]Management strategy and start up.

2.1. [bookmark: _Toc137798055][bookmark: _Toc229128258][bookmark: _Toc232953639][bookmark: _Toc516836507][bookmark: _Toc231566454][bookmark: _Toc231566580][bookmark: _Toc233624245]The Contractor’s plan for the service

The Contractor submits a bar (Gantt) chart plan in Excel format, detailing how the service is executed within the stipulated dates. The plan includes the following:
· Lead time from Contract start date to Site Establishment
· Working methods as well as details of the resources, including Equipment to be used
· Proposed time to complete each activity as per the scope of work.
· Links between activities indicating predecessors and successors.
· Health, Safety, Environmental, Quality and Security considerations (including 2 hours for site Safety Induction).
· Quality verification and testing activities.
· Key deliverable dates
· Breakdown of daily activities
· A financial cash flow projection shall be attached to the plan indicating the intended invoicing dates and amounts as for the entire contract period.
· The availability of materials intended for use, including the approval timeframe thereof, shall also be indicated on the plan.

The Contractor must submit with his tender, day work rates for all personnel, materials and equipment to be used in execution of the service

The plan will be subject to acceptance by the Employer and must be within the offered timeframes during
tender stage. 
The plan needs to be updated on daily basis and be available lo the Employer when required. The updated
plan must be presented to the Service Manager monthly and be part of the monthly progress meetings.

2.2. [bookmark: _Toc137798043][bookmark: _Toc229128246][bookmark: _Toc232953640][bookmark: _Toc516836508][bookmark: _Toc231566455][bookmark: _Toc231566581][bookmark: _Toc233624246]Management meetings

Regular meetings of a general nature may be convened and chaired by the Service Manager as follows:

	Title and purpose
	Approximate time & interval
	Location
	Attendance by:

	Kick-off meeting 
	Once-off
	Drakensberg Pumped Storage Scheme/Ms Teams
	Service Manager, Contractor, Employer and other relevant stakeholders 

	Progress and feedback meeting
	Quarterly 
	Drakensberg Pumped Storage Scheme/Ms Teams
	Contractor, Service Manager, Employer’s site support team

	Risk reduction meeting
	Ad hoc
	Drakensberg Pumped Storage Scheme/Ms Teams
	Service Manager, Contractor, Employer and other relevant stakeholders



Meetings of a specialist nature may be convened as specified elsewhere in this Service Information or if not so specified by persons and at times and locations to suit the Parties, the nature and the progress of the service.  Records of these meetings shall be submitted to the Service Manager by the person convening the meeting within five days of the meeting.  

All meetings shall be recorded using minutes or Ms Teams recordings or a register prepared and circulated by the person who convened the meeting.   Such minutes or register shall not be used for the purpose of confirming actions or instructions under the contract as these shall be done separately by the person identified in the conditions of contract to carry out such actions or instructions.  Attendees shall have the necessary delegated authority to make decisions in respect of matters discussed at each meeting.



2.3. [bookmark: _Toc137798049][bookmark: _Toc229128252][bookmark: _Toc232953641][bookmark: _Toc516836509][bookmark: _Toc231566456][bookmark: _Toc231566582][bookmark: _Toc233624247]Contractor’s management, supervision and key people

Contractor’s Management

· The Contractor provides adequate management resources to plan, monitor, and control the service.
· Management arrangements must demonstrate clear lines of responsibility and accountability.
· The Contractor submits an organisation chart showing reporting lines and management responsibilities. 
· The Contractor provides a detailed service organogram of the Company’s Branch, indicating specifically Operating officers, Communication/ liaison personnel and security staff intended for this contract.
· Changes in the service organogram must be communicated to the Service Manager immediately of it coming into effect.
· The Organogram includes contact details and emergency response (24-hour) information.

Supervision
· The Contractor ensures that the service is properly supervised at all times.
· Supervisor must be competent, experienced, and available on site during all working hours.
· The Contractor provides details of supervisory arrangements, including names, qualifications, and experience of supervisory staff.

Key People

· The following individuals are designated as Key People under the contract: 

· Contract/Project Manager
· Site Supervisor/ Pest Control Operator (PCO)
· Health & Safety Officer

· The Contractor provides CV’s and evidence of qualifications for each Key Person.
· Key People named in the contract may not be replaced without the Service Manager’s acceptance.
· Any proposed replacement must have equivalent qualifications and experience, and details must be submitted for approval prior to appointment.

Compliance & Reporting

· The Contractor notifies the Service Manager immediately of any changes to management, supervision, or Key People.
· Monthly reports shall be submitted confirming that management and supervision arrangements remain in place and effective.
· Failure to comply with these requirements may constitute a default under clause 91 of the NEC contract.

The Contractor employs in and about the Provision of the Services only such persons that are careful,
competent and efficient in their several trades and callings, to achieve safety excellence and highest quality standard

The Employer reserves the right to object to and require the Contractor to remove from the services, forthwith, any person employed by the Contractor in or about the Provision of the Services who, in the opinion of the Service Manager is incompetent, misconduct’s himself or negligent in the proper performance of his duties and such person is not again employed for the services without the written permission of the Service Manager.


2.4. [bookmark: _Toc137798044][bookmark: _Toc229128247][bookmark: _Toc232953643][bookmark: _Toc516836511][bookmark: _Toc231566457][bookmark: _Toc231566583][bookmark: _Toc233624248]Documentation control
2.4.1. [bookmark: _Toc180603498][bookmark: _Toc189655462][bookmark: _Toc195533946][bookmark: _Toc231566458][bookmark: _Toc231566584][bookmark: _Toc233624249]General

Each instruction, certificate, submission, proposal, record, acceptance, notification and reply is communicated in a form which can be read, copied and recorded and in the language of the Contract, within the period for reply or any other period agreed between the parties prior to its due date.  Any such communiqué must bear the signature of the author; emails therefore do not conform except when used as a transmittal medium.

2.4.2. [bookmark: _Toc180603499][bookmark: _Toc189655463][bookmark: _Toc195533947][bookmark: _Toc231566459][bookmark: _Toc231566585][bookmark: _Toc233624250]Minimum requirements
All documents shall be in simple and clear English; and always reference to applicable TSC clause under (or as a result of) which it is communicated.

2.4.3. [bookmark: _Toc180603500][bookmark: _Toc189655464][bookmark: _Toc195533948][bookmark: _Toc231566460][bookmark: _Toc231566586][bookmark: _Toc233624251]Use of standard forms
The Service Manager and the Contractor will use the standard TSC

2.4.4. [bookmark: _Toc180603501][bookmark: _Toc189655465][bookmark: _Toc195533949][bookmark: _Toc231566461][bookmark: _Toc231566587][bookmark: _Toc233624252]Communication
All Communication is addressed to the Service Manager as applicable to the TSC. All communication makes reference to:

· The Contract Number that is issued by the Employer (normally a 46000…..)
· The Contract title;
· Any previous reference relating to the specific communique;
· The specific TSC clause under which the communication is issued;
· Whether a reply is required and 
· A unique letter reference number.

The unique reference number to be used for written correspondence between the Service Manager and Contractor and vice versa is as follows:

· From the Service Manager to the Contractor: 46000...... E/C 0xxx; and from the Contractor to the Service Manager 46000         C/E 0xxx referring to the Contract number and the next sequential letter (channel) number

No contractual communication shall bypass the Service Manager unless explicitly stated in the contract.


2.5. [bookmark: _Toc232953644][bookmark: _Toc516836512][bookmark: _Toc231566462][bookmark: _Toc231566588][bookmark: _Toc233624253]Invoicing and payment

2.5.1. [bookmark: _Toc231566463][bookmark: _Toc231566589][bookmark: _Toc233624254] Invoice submission 

Within one week of receiving a payment certificate from the Service Manager in terms of core clause 51.1, the Contractor provides the Employer with a tax invoice showing the amount due for payment equal to that stated in the Service Manager’s payment certificate.  

The Contractor shall address the tax invoice to 

Eskom Holdings SOC Limited
P O Box 1091
Johannesburg
2000

and include on each invoice the following information:
· Name and address of the Contractor and the Service Manager;
· The contract number and title;
· Contractor’s VAT registration number;
· The Employer’s VAT registration number: 4740101508;
· Total amount invoiced excluding VAT, the VAT and the invoiced amount including VAT;
· Contractor's company registration number if applicable
· Contractor’s banking details
· Tax invoice number and date of issue,
· Description and quantity of goods/service provided,
· Contract Number (commencing with a 46 prefix)
· Relevant Purchase Order Number (commencing with a 45 prefix),
· Relevant line item number,
· Relevant goods receipt / service entry number received from the Employer's Service Manager

All invoices to be accompanied by the Payment Assessment Certificate as issued by the Service Manager. Invoices must be submitted electronically as PDF documents to:
  	Local Eskom Invoices - invoiceseskomlocal@eskom.co.za
Failure to submit the invoice to the correct address could result in delays in payment. 

[bookmark: _Toc231566464][bookmark: _Toc231566590][bookmark: _Toc233624255]2.5.2.   How to submit invoices
[bookmark: _Toc231566465][bookmark: _Toc231566591][bookmark: _Toc233624256]a) General Submission Information 
•	The subject line on your email should only contain your Eskom vendor number.
•	Each invoice in PDF should be named with your invoice number only.
•	Ensure that the Eskom task order number is clearly indicated on your invoice together with the line number you are billing for.
•	Ensure you comply with the SARS tax requirements for submitting invoices electronically.
•	Each PDF files should contain one invoice, one debit note, or one credit note only. You may submit more than one invoice per email.
•	All electronic invoices must be sent in PDF format only.
•	Attach proof of delivery to your invoice (eg assessment certificate).
•	Where applicable, supporting documents must be attached to the scanned PDF invoice as one attachment.
o	Assessment Certificate / delivery note.
o	CPA calculation sheet.
o	Retention certificates where it is a retention invoice.
o	Any other appropriate documents.

[bookmark: _Toc231566466][bookmark: _Toc231566592][bookmark: _Toc233624257]b) 	CPA
CPA is applied as per Secondary Option X1 in Contract Data. If there is CPA on your invoice, it is must be issued as a separate invoice for CPA, so that if there is any issues on the CPA , the base invoice can be paid whilst CPA issues are resolved.
CPA calculation sheets must accompany the invoice.

2.5.2. [bookmark: _Toc184584763][bookmark: _Toc222246368][bookmark: _Toc231566467][bookmark: _Toc231566593][bookmark: _Toc233624258]Payment Queries
For all queries and follow-ups on payments, kindly contact the Finance Shared Services Contact Centre
· Tel: 011 800 5060
· Email: fss@eskom.co.za
2.5.3. [bookmark: _Toc184584764][bookmark: _Toc222246369][bookmark: _Toc231566468][bookmark: _Toc231566594][bookmark: _Toc233624259]Eskom information
· Eskom Tax clearance and BBBEE certificate is available at: https://www.eskom.co.za/Tenders/BBBEECertificate/Pages/Eskom_BBBEE_Certificate.aspx
· Eskom VAT  Number is 4740101508 
2.5.4. [bookmark: _Toc184584765][bookmark: _Toc222246370][bookmark: _Toc231566469][bookmark: _Toc231566595][bookmark: _Toc233624260]Avoid Payment Delays
· Failure to submit a PDF invoice with accompanying assessment electronically to Invoiceseskomlocal@eskom.co.za could result in payment delays.
· Contractor to ensure the  Service Manager  has an updated valid certified copy of BBBEE certificate or sworn affidavit, tax certificate and Letter of Good standing during contract period.. Failure to do so, could result in Eskom Vendor Management Dept blocking vendor details on Eskom vendor management system which affects payment processing of invoices.
· It is important that the value stated on the invoice must be the same as the value stated on the task order. If the invoice value is different from the task order value, payment of the invoice will be delayed. It is strongly recommended that if there are any discrepancies on the invoice, it will be rectified with the Service Manager before it is submitted for payment.
Ensure remittance email address and name on invoice are correct and that Eskom has received the same information to update its records. If different in Eskom’s system, it will delay processing of invoice.


2.6. [bookmark: _Toc137798052][bookmark: _Toc229128255][bookmark: _Toc232953645][bookmark: _Toc516836513][bookmark: _Toc231566470][bookmark: _Toc231566596][bookmark: _Toc233624261]Contract change management 

As prescribed by the NEC3. 

2.7. [bookmark: _Toc137798054][bookmark: _Toc229128257][bookmark: _Toc232953646][bookmark: _Toc516836514][bookmark: _Toc231566471][bookmark: _Toc231566597][bookmark: _Toc233624262]Records of Defined Cost to be kept by the Contractor

The Contractor is required to keep a clear and auditable format for the purpose of compensation event management. The Service Manager has the right to inspect these records at any time. Costs not properly evidenced may be treated as Disallowed Cost. These records need to be available on a spreadsheet in case a compensation event is agreed on.

Records of Defined Cost

· Labour Costs
· Timesheets showing hours worked.
· Payroll records (wages, salaries, overtime, allowances).
· Evidence of statutory contributions (e.g., pensions, insurance, taxes).

· Plant and Equipment
· Hire agreements and invoices.
· Logs of usage hours or days.
· Maintenance and running costs.

· Materials
· Purchase orders and invoices.
· Delivery notes and stock records.
· Waste or surplus documentation.

· Subcontractors
· Subcontract agreements.
· Payment certificates and invoices.
· Records of work done and progress.

· Other Defined Costs
· Travel expenses (tickets, mileage logs).
· Accommodation costs.
· SHE related


2.8. [bookmark: _Toc137798051][bookmark: _Toc229128254][bookmark: _Toc232953647][bookmark: _Toc516836515][bookmark: _Toc231566472][bookmark: _Toc231566598][bookmark: _Toc233624263]Insurance provided by the Employer

As per Clause Z12, Queries regarding insurance claims and/or procedures can be addressed with the Service Manager.


2.9. [bookmark: _Toc137798062][bookmark: _Toc229128265][bookmark: _Toc232953650][bookmark: _Toc516836518][bookmark: _Toc231566473][bookmark: _Toc231566599][bookmark: _Toc233624264]Things provided at the end of the service period for the Employer’s use
[bookmark: _Toc516836519][bookmark: _Toc231566474][bookmark: _Toc231566600][bookmark: _Toc233624265]Equipment
None 
[bookmark: _Toc516836520][bookmark: _Toc231566475][bookmark: _Toc231566601][bookmark: _Toc233624266]Information and other things
At the end of the service period or earlier termination of this contract, the Contractor shall make available to the Employer all records and information relating to the service carried out under this contract at no extra cost to the Employer excluding the Contractors intellectual property.


2.10. [bookmark: _Toc232953651][bookmark: _Toc516836521][bookmark: _Toc231566476][bookmark: _Toc231566602][bookmark: _Toc233624267]Management of work done by Task Order


Tree felling

Tree felling service is done on an “as and when required” basis, instructed via Task Order process. The Service Manager issues a Task Order to the Contractor which clearly specifies the number of trees to be worked on, additional SHEQ specification; procedures; any other constraints the Contractor complies with in providing the service.
. 
Within Five (5) days of receiving the Task Order, the Contractor submits the following to the Service Manager for acceptance: 

· Quotation for carrying out the task, the quotation includes breakdowns of costs, resources and timelines.  .
· Task Order programme showing all the information required by Clause X19.6 of NEC3 TSC.
· Additional OHS requirements as specified in the Task Order
· Any other requirement as specified in the Task Order

This process requires the Employer’s intervention to verify if the quotation is fair and reasonable. This involves checking against benchmarks, market rates, and contract provisions. The Employer may request clarifications or adjustments from the Contractor. The Employer may negotiate or reject the quotation. Once the Employer confirms the quotation is fair and reasonable, the Service Manager issues the formal task order instruction commencing with a 45 number. This authorizes the Contractor to proceed with the service.


Supply of indigenous trees for Arbor Day celebration

The service is instructed through a Task Order process. The Service Manager requests the Contractor to quote for three specific indigenous trees. The Contractor provides quote for the Employer’s review. The Employer verifies if the quotation is fair and reasonable. The Employer may request clarifications or adjustments from the Contractor. The Employer may negotiate or reject the quotation. Once the Employer confirms the quotation is fair and reasonable, the Service Manager issues the formal task order instruction commencing with a 45 number. This authorizes the Contractor to proceed with the service.


3. [bookmark: _Toc232953652][bookmark: _Toc516836522][bookmark: _Toc231566477][bookmark: _Toc231566603][bookmark: _Toc233624268]Health and safety, the environment and quality assurance
3.1. [bookmark: _Toc231566478][bookmark: _Toc231566604][bookmark: _Toc233624269][bookmark: _Ref134768869][bookmark: _Toc137798045][bookmark: _Toc229128248][bookmark: _Toc232953653][bookmark: _Toc516836523]Occupational Health and Safety 

3.1.1. The Contractor shall comply with the health and safety requirements contained in OHS Requirements and the approved safety file by Eskom. Eskom reserves the right to review the OHS Requirements to address the Operational risks and the contractor shall comply with the latest OHS Requirements as amended at no cost for the duration of the contract on the Affected Property as listed in section 11.2(2).
3.1.2. The section 37(2) agreement as stipulated under the OHS Act no 85 of 1993 must be signed by Contractor and Employer representatives.
3.1.3. The Contractor OHS professional must conducts internal audits at planned intervals (for the duration of the contract at the Affected Property as listed in section 11.2(2) to monitor compliance to the contractual health and safety requirements.
3.1.4. The Service Manager/Contract Manager must conduct inspections at planned intervals (for the duration of the contract at the Affected Property as listed in section 11.2(2) to monitor compliance to the contractual health and safety and legal requirements. 
3.1.5. The Contractor may be selected during internal and/or external Peaking Power Station audits to verify compliance to legal and contractual OHS requirements. The Contract Manager/Service Manager will communicate this at relevant time periods and the Contractor shall avail themselves for this audit.
3.1.6. In addition to the requirements of the applicable laws governing the occupational health and safety, Peaking Power Station OHS requirements particular to the service and the Affected Property as listed in section 11.2(2) for this contract shall be adhered to for the duration of the contract.
3.1.7. The minimum requirements for the Contractor to gain access to Peaking Power Station include the but not limited to:
· Valid Medical fitness certificate
· Police clearance from SAPS or accredited supplier/service provider linked to SAPS AFIS system not older than thirty (30) days. 
· Identification document (RSA ID or equivalent)
· National Drivers Licence (applicable to drivers)
· Adherence to the Eskom Life-saving rules 3 and 4, Be Sober and Buckle up
	Rule
	Description of rule

	3
	BUCKLE UP
No person may drive any vehicle on Eskom business and/or on Eskom premises:
Unless the driver and all passengers are wearing seat belts

	4
	BE SOBER
No person is allowed to be under the influence of intoxicating liquor or drugs while on duty


· Applicable risk-based PPE.
· Valid letter of good standing always (COIDA or equivalent). Access to site to perform work will be denied should the Letter of good standing not be valid.
· The Contractor/supplier/consultant who is working alone and not eligible to register with the compensation fund, shall provide Eskom with the member benefit statement of the insurance cover which include life and disability cover to the minimum fund of R500 000.
Note: Induction will only be conducted after the above documents have been submitted and accepted by Eskom.
3.1.8. [bookmark: _Toc184584772][bookmark: _Toc222246377]Contractor Management Key Performance Indicators
· Maintain Health and Safety file and compliance to the health and safety plan, Eskom OHS requirements and applicable legislation as amended. 
· Always maintain good housekeeping where the task is being executing and/or within the area of responsibility.
· Implement and monitor near miss reporting strategy / programme (reporting of near misses). 
· Develop and comply to Behavioural Safety Observation (BSO) and Planned Job Observation programmes (PJO).
· Maintain Zero Fatalities for the duration of the contract.
· At any given point, the OHS performance must be within the lost time injury (LTI) tolerance level as amended.
· All incidents must be reported immediately or before the end of the particular shift during which the incident occurred.
· All incident investigations shall be completed within 30 days of the occurrence of an incident.
· Incident investigation recommendations shall be closed within the recommended time frame recorded in the Incident investigation report.
· Close audit findings as per the Eskom procedure or audit report recommended time frames. 
· Close Non-conformance as per the recommended time frames.
Note: Monitoring of the above mentioned KPI’s will take place through regular audits and inspection.


3.1.9. Main contractors


· Carry out all duties as listed in section 8, 9 and 10, of the OHS Act and Regulations. 
· Carry accountability and responsibility for the safety and health of his employees and their appointed contractors within their working area, as contemplated by section 37(2) of the OHS Act;
· The Contractor keeps a record of all his  employees, including date of induction, relevant skills and licenses and be able to produce this list at the request of the Service Manager. 
· Ensures that all their appointees are made aware of their accountabilities and responsibilities in terms of their appointment and that they advise and assist these appointees in the execution of their duties. 
· Ensures that the minimum legislative, regulatory and Eskom SHE requirements are complied with on all work sites. 
· Give the Service Manager and other line managers/responsible managers full participation and cooperation when required. 
· Compiles a SHE (health and safety) file where all relevant health and safety records must be kept for the Affected Property. 
· The Contractor provides the Service Manager with the Compensation Commissioner’s valid letter of good standing before the commencement of work and any future renewal letters obtained during the contract for record-keeping purposes. The letter of good standing shall reflect the name of the contractor’s company. Similarly, the Contractor must provide the Service Manager with all the valid letters of good standing for his subcontractors. 
· The subcontractor’s provides the Contractor with the Compensation Commissioner’s valid letter of good standing before the commencement of work and any future renewal letters obtained during the contract for record-keeping purposes. The letter of good standing shall reflect the name of the Contractor’s  company. 
· The Contractor appoints competent staff to perform for the service and ensure that all employees are trained in the health and safety aspects relating to such servive and that the employees understand the hazards associated with all other work being carried out on the project. 
· Ensures that all employees are conversant with all relevant work procedures and that they adhere to such procedures. Similarly (without removing the appointed contractors’ responsibilities), ensure that their appointed contractors and their employees are conversant with all relevant work procedures and that they adhere to such procedures.
· Co-ordinates the activities of all his subcontractors in the interests of safety and health; 
· Ensures that their contractors (whom they intend appointing) have made detailed provision for the cost of safety and health measures throughout the project. 
· Stops his employees and his subcontractors if such work poses a threat to the health and safety of persons or a risk of degradation to the environment. 
· Takes reasonable steps to ensure cooperation between all their appointed contractors. 
· The Contractor ensures that Employer’s OHS requirements are communicated to all his subcontractors, evaluate, and assess the subcontractors OHS files. Only appoint sbcontractors who are competent to do work, have satisfied the OHS compliance requirements and satisfied that the contractor has the necessary competencies and resources to perform the work safely 
· The Contractor appoints full-time competent employees in writing to supervise the performance of all specified work throughout the contract period. 
· The Contractor ensures that the contract supervisor does not supervise work on any site other than the Affected Property for which such supervisor has been appointed for. 
· Does not victimise or dismiss employees, by virtue of the employees divulging health and safety information or suspecting such information has been divulged, in the interests of health and safety requirements; 
· The Contractor follows a process of disciplinary action if any of his employees or his subcontractor employees have transgressed any of the requirements of the health and safety specification, safety and health plans, site rules or any other requirements. 
· Before the commencement of work, review the submitted baseline risk assessments to include site or emerging risks. This should be done by a competent person appointed in writing with a view to identify hazardous and potentially hazardous work operations. 
· Ensures that pre-task risk assessments are conducted and documented daily and prior to the starting of any new task, irrespective of whether it is a repetitive task or not. 
· The Contractor ensures that an organisation medical surveillance programme for the duration of the contract is in place and maintained. 
· Prior to having pre-employment and periodic medicals fitness examinations conducted, person/man job specifications must be compiled and handed to the occupational health practitioner. 
· Issues risk-based personal protective equipment (PPE) as a measure of last resort to their employees, inspect such equipment regularly and ensure recipients of PPE are trained in the proper use, care and where necessary, the maintenance of PPE; Note: should the main contractor or his/her appointed contractors entertain visitors on site, they will be held responsible for the provision and wearing PPE.
· The Contractor have a substance abuse program which in line with Employer’s requirements. 
· Ensures that all incidents are reported and investigated timeously by competent incident investigators and aligned with 32-95 requirements. 
· Is involved in all his subcontractor’s incident investigations. 
· For subcontracted work, the Contractor advises the Service Manager in writing timeously and obtain his accaptance prior to subcontractor’s appointment and the work commencement thereof. 



3.1.10. Contractor site supervisor

The Contractor supervisor is trained on the following: 

· HIRA
· Incident investigation
· Legal liability Training
· Supervisor Training
The Contractor supervisor

· Is competent to perform the required supervisory tasks. 
· Ensures the Contractor employees comply with the required statutory and Eskom project requirements. 
· Inspects all work done to ensure adherence to Employer’s standards and specifications. 
· Conducts follow-up inspections to ensure findings are closed out and preventative action is in place. 
· Monitors contractors for adhere to statutory requirements and safety standards. 
· Monitor contractors overall SHE performance on site in order to achieve excellent results. 
· Discuss all SHE related problems with the relevant contractor management timeously in the first instance and thereafter the Service Manager in the second instance relating to procedure requirements, non-conformance’s identified, corrective actions, audits and inspection schedules. 
· Continual liaison between the main contractor, appointed contractors and employees. 
· Ensures that employees and subcontractors are aware of latest standards, procedures, work instructions and safety regulations issued by Eskom: 




3.2. [bookmark: _Toc231566479][bookmark: _Toc231566605][bookmark: _Toc233624270][bookmark: _Toc137798046][bookmark: _Toc229128249][bookmark: _Toc232953654][bookmark: _Toc516836524]Key Performance Indicators
3.2.1. Contractor/Supplier Management Key Performance Indicators (KPI’s)
3.2.2. Maintain Health and Safety file and compliance to the health and safety plan, Eskom OHS requirements and applicable legislation as amended. 
3.2.3. Always maintain good housekeeping where the task is being executing and/or within the area of responsibility.
3.2.4. Implement and monitor near miss reporting strategy / programme (reporting of near misses). 
3.2.5. Develop and comply to Behavioural Safety Observation (BSO) and Planned Job Observation programmes (PJO).
3.2.6. Maintain Zero Fatalities for the duration of the contract.
3.2.7. At any given point, the OHS performance must be within the lost time injury (LTI) tolerance level as amended.
3.2.8. All incidents must be reported immediately or before the end of the particular shift during which the incident occurred.
3.2.9. All incident investigations shall be completed within 30 days of the occurrence of an incident.
3.2.10. Incident investigation recommendations shall be closed within the recommended time frame recorded in the Incident investigation report.
3.2.11. Close audit findings as per the Eskom procedure or audit report recommended time frames. 
3.2.12. Close Non-conformance as per the recommended time frames.
Note: Monitoring of the above mentioned KPI’s will take place through regular audits and inspection.
3.3. [bookmark: _Toc184584773][bookmark: _Toc222246378][bookmark: _Toc231566480][bookmark: _Toc231566606][bookmark: _Toc233624271]Contract completion and sign off
On completion of the project/contract, Eskom team (led by the Contract Manager) involved in the project together with the Contractor shall conduct the final meeting to identify the gaps prior to the contract close out. Before the final invoice is paid/processed, the Contract Manager shall ensure that the below requirements are met:
3.3.1. Close all incidents and audit findings.
3.3.2. Clean the respective area and ensure good housekeeping where the contractor was working.
3.3.3. Contractor shall submit safety statistics and a safety file to Eskom Safety Department for closeout and filling. 
3.3.4. Completion of a closeout report (Annexure D form as per 32-726) to close the contractual work.

3.4. [bookmark: _Toc231566481][bookmark: _Toc231566607][bookmark: _Toc233624272]Environmental constraints and management

The Contractor’s rates tendered shall cover all costs that will be incurred to comply with all requirements of the environmental requirements. Special attention is drawn inter alia to the following aspects:
· The Contractor’s attention is drawn to the fact that the Power Station is situated in a highly sensitive environmental area and that any incident that may result in an environmental impact must be brought to the attention of the Service Manager as soon as it is possible. The site is managed in accordance with an ISO 14001 certified management system, and the contractor will be expected to manage all processes in line with environmentally sound principles. 
· The following environmental requirements are always complied with:
· Zero liquid effluent discharge.
· No chemicals will be dumped into the station drains or on the premises.
· No oil or waste will be dumped in an unauthorised area or unlicensed waste site.
· Asbestos will be handled and stored according to Act 15 of 1973 (hazardous substances Act).
· No materials or waste will be burnt on site.  Hazardous substances shall be handled and stored according to the hazardous substances Act no 15 of 1973.  No effluent shall be discharged into the public streams.
· Construction Safety, Health, and Environmental Management Rev 0 32-136
· The Contractor, in and about the execution of the service, complies with all applicable national, provincial and Municipal environmental legislation and by laws. 
· Comply with all environmental legislation of South Africa, including but not limited to:
National Environmental Management Act 107 of 1998 
National Environmental Management Waste Act 59 of 2008
National Water Act 36 of 1998
Eskom Waste Standard latest revision
Waste Management: Norms and standards: Act 59 of 2008 latest revision
· The Contractor shall comply to all National and Local legislation requirements as well as Eskom procedures and policy. Eskom’s goal is to ensure zero harm to the environment, and to ensure that any possible impact is mitigated or managed.  The Duty of Care and implementation of best practice is critical during operations, and full communication on environmental issues is required at all times.
· Site/laydown demarcation: The Contractor shall demarcate his camp site, be restricted to that specific area and take full responsibility to restore the area to its original condition before the contract commenced. 
·  Waste management: The Contractor shall dispose of all waste off-site at a licensed waste disposal facility and submit proof to Eskom. The method statement on waste management will need to include the identification of possible waste streams, temporary storage and disposal options for each waste type, and contingency plans in the case of any environmental incident. A Safety Data Sheet must be supplied for all chemical or hazardous / potentially hazardous material brought onto site.”
· Sanitation: The Contractor shall provide an appropriate enclosed temporary sanitation facility 
· Dust control: The Contractor shall be responsible to apply effective dust control measures.
· Fire prevention: It shall be the responsibility of the Contractor to prevent fires at all times during the contract.
· The Contractor shall take full responsibility for protecting the natural environment and eliminating or minimising the negative impacts of construction on the environment during construction. Nothing specified herein shall relieve the Contractor of any obligations or responsibilities in this regard.
· If product is classified as a hazardous substance, safety brochures must accompany delivery. In accordance with the Occupational Health and Safety Act (OHSA), Act 85 of 1993 section 10 and 11.  If any hazard is identified by the Contractor, he must immediately inform the Employer.


3.5. [bookmark: _Toc137798047][bookmark: _Toc229128250][bookmark: _Toc232953655][bookmark: _Toc516836525][bookmark: _Toc231566482][bookmark: _Toc231566608][bookmark: _Toc233624273]Quality assurance requirements

Quality management for the Works is under Eskom Supplier Quality Management Specification 240-105658000 (QM-58).

The quality requirements applicable to this contract are captured in the Supplier Quality Management
Specification QM 58 (240-105658000) category 4, which specify and describe the main quality criteria for the
selection, evaluation, registration, monitoring and auditing of Contractors. This specification as provided during tender will be seen as part of the services. It will work hand in hand with category 4 (Form A) Tender & Contract Quality Requirements for QM58 and Quality requirements for ISO 9001 Standard. A Quality Control Plan/Inspection and Test Plan template as well as a Template for Typical Contract Quality Plan will be provided

The Contractor defines the level of QA/QC or inspection imposed on his sub-contractors where applicable
 
The programming of inspection, hold and witness points agreed between the Employer and the Contractor
prior to undertaking any work.
 
The Contractor arranges, supervise and monitor services as per the agreed specification and work procedures approved by the Employer. All services to be carried out by qualifies persons
3.5.1. [bookmark: _Toc170121507][bookmark: _Toc172801206][bookmark: _Toc184584777][bookmark: _Toc222246382][bookmark: _Toc231566483][bookmark: _Toc231566609][bookmark: _Toc233624274]Quality Control Plan
The Quality Plan manages the overall quality of the project’s main activities and milestones. It lists detailed activities in order of execution where each activity is described and references the associated work packages or specifications with witness, hold and verification points.
The Contractor is therefore required to ensure QCPs meet the following requirements as a minimum:
a) The Contractor defines the level of QC or inspection imposed on his subcontractors and suppliers. 
b) The QCPs are to have provisions for signatures indicating Completion by the Contractor and acceptance by the Employer at the end of each activity. 
c) The Contractor has the necessary Equipment and qualified staff to carry out the quality control required to ensure compliance with the specification. 
d) The Contractor ensures that a complete Quality Control Plan (QCP) aligned with the Method Statement, and program for executing the work, is submitted to the Service Manager and Supervisor for review and acceptance before the Works can commence. 
e) The programming of inspections, hold and witness points are agreed between the Employer and the Contractor before undertaking any of the Works. 
f) During reviews of the QCP, the Employer provides the necessary intervention points, if required.

4. [bookmark: _Toc137798064][bookmark: _Toc229128267][bookmark: _Toc232953656][bookmark: _Toc516836526][bookmark: _Toc231566484][bookmark: _Toc231566610][bookmark: _Toc233624275]Procurement
[bookmark: _Toc137798065][bookmark: _Toc229128268][bookmark: _Toc232953657][bookmark: _Toc516836527]
4.1. [bookmark: _Toc231566485][bookmark: _Toc231566611][bookmark: _Toc233624276]People
4.1.1. [bookmark: _Toc137798066][bookmark: _Toc229128269][bookmark: _Toc232953658][bookmark: _Toc516836528][bookmark: _Toc231566486][bookmark: _Toc231566612][bookmark: _Toc233624277]Minimum requirements of people employed
The Contractor provides a detailed Curriculum Vitae (CV) containing qualifications, skills, competencies, and experience with certified copies of qualifications and certificates, from a recognised South African body e.g. SETA, SAQA etc. People with non-South African qualifications need to have their qualifications verified by SAQA and a Certification of Evaluation issued. The Contractor shall ensure that the staff has the necessary training including but not limited to Chainsaw Operator, Herbicide Applicator, Brush Cutter Operator and Snake Handling. The following are required
 
· Part time Safety Officer - The Safety Officer is qualified (holds an OHS Diploma) and trained on SAMTRAC, HIRA, Incident investigation training, Legal liability Training, and has a knowledge and understanding of ISO 4500, Minimum work experience 2yrs, OHS Diploma (applicable to 3-5 years contract)
· Contractor site supervisor and PCO
· 9 x General workers 

4.1.2. [bookmark: _Toc137798067][bookmark: _Toc229128270][bookmark: _Toc232953659][bookmark: _Toc516836529][bookmark: _Toc231566487][bookmark: _Toc231566613][bookmark: _Toc233624278]BBBEE and preferencing scheme
The Contractor to ensure the Service Manager has an updated valid certified copy of BBBEE certificate or sworn affidavit during contract period. Failure to do so, could result in Eskom Vendor Management Department blocking vendor details on Eskom vendor management system which affects payment processing of invoices.

4.1.3. [bookmark: _Toc231566488][bookmark: _Toc231566614][bookmark: _Toc233624279]Supplier Development, Localisation and Industrialisation (SDL&I)
Information to be inserted after negotiation stage. 

4.2. [bookmark: _Toc137798068][bookmark: _Toc229128272][bookmark: _Toc232953661][bookmark: _Toc516836531][bookmark: _Toc231566489][bookmark: _Toc231566615][bookmark: _Toc233624280]Subcontracting
4.2.1. [bookmark: _Toc137798069][bookmark: _Toc229128273][bookmark: _Toc232953662][bookmark: _Toc516836532][bookmark: _Toc231566490][bookmark: _Toc231566616][bookmark: _Toc233624281]Preferred subcontractors
No Nominated Subcontractors

4.2.2. [bookmark: _Toc137798070][bookmark: _Toc229128274][bookmark: _Toc232953663][bookmark: _Toc516836533][bookmark: _Toc231566491][bookmark: _Toc231566617][bookmark: _Toc233624282]Subcontract documentation, and assessment of subcontract tenders
It is compulsory for the Contractor to use NEC system when subcontracting. The Contractor does
not appoint a proposed Subcontractor until the Service Manager has accepted him.

4.2.3. [bookmark: _Toc137798071][bookmark: _Toc229128275][bookmark: _Toc232953664][bookmark: _Toc516836534][bookmark: _Toc231566492][bookmark: _Toc231566618][bookmark: _Toc233624283]Limitations on subcontracting
None. 


4.2.4. [bookmark: _Toc137798072][bookmark: _Toc229128276][bookmark: _Toc232953665][bookmark: _Toc516836535][bookmark: _Toc231566493][bookmark: _Toc231566619][bookmark: _Toc233624284]Attendance on subcontractors
[bookmark: _Hlk178750490]It is the sole responsibility of the Contractor.



4.3. [bookmark: _Toc137798073][bookmark: _Toc229128277][bookmark: _Toc232953666][bookmark: _Toc516836536][bookmark: _Toc231566494][bookmark: _Toc231566620][bookmark: _Toc233624285]Plant and Materials
4.3.1. [bookmark: _Toc516836537][bookmark: _Toc231566495][bookmark: _Toc231566621][bookmark: _Toc233624286]Specifications
All materials and equipment required and necessary to provide services by the Contractor on the Affected Property shall be carefully selected and tested by the Contractor before actual performance of services in the Affected Property.

4.3.2. [bookmark: _Toc516836538][bookmark: _Toc231566496][bookmark: _Toc231566622][bookmark: _Toc233624287]Correction of defects
The Contractor provides a report detailing the nature of the defective area, the report should also give recommendations as to whether the defect can be fixed or not. The Employer is entitled to witness the defective area. 

No replacement of vegetation must be done without an instruction by the Service Manager. 

4.3.3. [bookmark: _Toc137798076][bookmark: _Toc229128280][bookmark: _Toc232953669][bookmark: _Toc516836539][bookmark: _Toc231566497][bookmark: _Toc231566623][bookmark: _Toc233624288]Contractor’s procurement of Plant and Materials
The Contractor provides the Service Manager with a quotation with the agreed markup percentage for all materials, vegetation or specialised services required to perform repairs. The Contractor attaches the Vendor’s invoice or proof of purchase together with the Contractor’s quotation as supporting evidence. The warrantees from suppliers are to be in favour of the Employer and not just the Contractor. 

4.3.4. [bookmark: _Toc137798078][bookmark: _Toc229128282][bookmark: _Toc232953671][bookmark: _Toc516836540][bookmark: _Toc231566498][bookmark: _Toc231566624][bookmark: _Toc233624289]Tests and inspections before delivery
Where applicable calibration certificates, pressure test certificates etc, are required for parts and equipment supplied by the Contractor.

4.3.5. [bookmark: _Toc137798075][bookmark: _Toc229128279][bookmark: _Toc232953668][bookmark: _Toc516836541][bookmark: _Toc231566499][bookmark: _Toc231566625][bookmark: _Toc233624290]Plant & Materials provided “free issue” by the Employer
None. All other Plant and Materials are to be provided by the Contractor.


4.3.6. [bookmark: _Toc516836542][bookmark: _Toc231566500][bookmark: _Toc231566626][bookmark: _Toc233624291]Cataloguing requirements by the Contractor
None. 


5. [bookmark: _Toc232953672][bookmark: _Toc516836543][bookmark: _Toc231566501][bookmark: _Toc231566627][bookmark: _Toc233624292]Working on the Affected Property
5.1. [bookmark: _Toc137798084][bookmark: _Toc229128287][bookmark: _Toc232953673][bookmark: _Toc516836544][bookmark: _Toc231566502][bookmark: _Toc231566628][bookmark: _Toc233624293]Employer’s site entry and security control, permits, and site regulations
All persons intending to perform work and/or attend meetings during this contract period at Affected Property have to comply with the following:
•	Each person shall sign the entrance register and this information shall also be collated by the Contractor for use during the scheduled meetings.
•	All persons entering the premises might be required to undergo a breathalyser test. Any persons testing positive will not be allowed entry. The Employer has a zero tolerance towards alcohol.
The Contactor to adhere to Drakensberg Pumped Storage Scheme’s Security Control measures and entry requirements.


5.2. [bookmark: _Toc137798086][bookmark: _Toc229128289][bookmark: _Toc232953674][bookmark: _Toc516836545][bookmark: _Toc231566503][bookmark: _Toc231566629][bookmark: _Toc233624294]People restrictions, hours of work, conduct and records

The Contractor upholds Eskom’s Code of Ethics.

An attendance register will be required to be completed and retained by the Contractor.
Working Hours:
•	Mon – Thursday: 07H300 - 16H15
•	Fridays: 07H00 - 12H00
Lunch time:
•	Monday – Thursday: 12H00 to 12H30
•	Friday: None

5.3. [bookmark: _Toc137798087][bookmark: _Toc229128290][bookmark: _Toc232953675][bookmark: _Toc516836546][bookmark: _Toc231566504][bookmark: _Toc231566630][bookmark: _Toc233624295]Health and safety facilities on the Affected Property

Refer Section 3.1. 

5.4. [bookmark: _Toc137798088][bookmark: _Toc229128291][bookmark: _Toc232953676][bookmark: _Toc516836547][bookmark: _Toc231566505][bookmark: _Toc231566631][bookmark: _Toc233624296]Environmental controls, fauna & flora

Refer Section 3.4.

5.5. [bookmark: _Toc137798090][bookmark: _Toc229128293][bookmark: _Toc232953677][bookmark: _Toc516836548][bookmark: _Toc231566506][bookmark: _Toc231566632][bookmark: _Toc233624297]Cooperating with and obtaining acceptance of Others

Proper co-ordination and work planning must be done when working in any area and where others are also performing work or activities. Interfacing is required with the office staff and other Contractors. As per clause 25 of TSC 3

5.6. [bookmark: _Toc137798092][bookmark: _Toc229128295][bookmark: _Toc232953678][bookmark: _Toc516836549][bookmark: _Toc231566507][bookmark: _Toc231566633][bookmark: _Toc233624298]Records of Contractor’s Equipment

The Contractor shall, before entering the office for the first time, provide a comprehensive list of all equipment and tools intended for use during the contract period, to the Service manager. 

5.7. [bookmark: _Toc137798093][bookmark: _Toc229128296][bookmark: _Toc232953679][bookmark: _Toc516836550][bookmark: _Toc231566508][bookmark: _Toc231566634][bookmark: _Toc233624299]Equipment provided by the Employer

Electricity plug points in areas of the Affected Property where electricity is available and only when there is no loadshedding (during this time the Contractor must provide its own energy source).


5.8. [bookmark: _Toc137798094][bookmark: _Toc229128297][bookmark: _Toc232953680][bookmark: _Toc516836551][bookmark: _Toc231566509][bookmark: _Toc231566635][bookmark: _Toc233624300]Site services and facilities
5.8.1. [bookmark: _Toc232953681][bookmark: _Toc516836552][bookmark: _Toc231566510][bookmark: _Toc231566636][bookmark: _Toc233624301]Provided by the Employer
First Aid facilities: Not Available. 
Ablution facilities: Available.

5.8.2. [bookmark: _Toc137798095][bookmark: _Toc229128298][bookmark: _Toc232953682][bookmark: _Toc516836553][bookmark: _Toc231566511][bookmark: _Toc231566637][bookmark: _Toc233624302]Provided by the Contractor
The Contractor provides the necessary labour, Personal Protective Equipment (PPE), home-work-home transport, meals, and accommodation that will satisfy the requirements of this contract.
The Contractor provides all the tools and equipment required to satisfy the requirements of this contract.
The Contractor provides all the materials, spares and/or parts necessary to satisfy the requirements of this contract.
The Contractor provides everything else necessary for providing the Service.

· The Contractor shall provide vehicles for use by the Service Manager and Employer’s staff where specified.
· Vehicles must be roadworthy, insured, and maintained in accordance with statutory requirements.
· Equipment must be maintained in good working order and replaced if defective.
· Consumables (paper, ink, etc.) shall be supplied by the Contractor.
· Contractor’s own facilities (accommodation, storage, vehicles, laboratories) must meet minimum standards set out in the Scope.
· Facilities must comply with health, safety, and environmental regulations.
· Upon completion of the contract, facilities provided by the Contractor shall be: 
Removed from the site if temporary and Contractor-owned.
Handed over to the Employer if specifically procured for Employer use and ownership transfer is stated in the Scope.
· The Contractor shall restore any areas used for temporary facilities to their original condition unless otherwise agreed.



5.9. [bookmark: _Toc137798100][bookmark: _Toc229128303][bookmark: _Toc232953683][bookmark: _Toc516836554][bookmark: _Toc231566512][bookmark: _Toc231566638][bookmark: _Toc233624303]Control of noise, dust, water and waste 

Offices are occupied by employees performing their work during normal hours. Any disruptions to these employees must be avoided and where not possible kept to a minimum. The Contractor shall take all necessary precautions to control noise to a minimum.

5.10. [bookmark: _Toc232953685][bookmark: _Toc516836556][bookmark: _Toc231566513][bookmark: _Toc231566639][bookmark: _Toc233624304]Tests and inspections
5.10.1. [bookmark: _Toc232953686][bookmark: _Toc516836557][bookmark: _Toc231566514][bookmark: _Toc231566640][bookmark: _Toc233624305]Description of tests and inspections
Inspections will be carried out by the Health & Safety Officer, the Environmental officer and the Service Manager periodically.  This information will be shared during meetings.
Inspections carried out by the Contractor, specifically those intended for the prevention of harbouring areas, must be recorded and recommendations communicated with the Service Manager as soon as it becomes apparent.



6. [bookmark: _Toc137798122][bookmark: _Toc229128325][bookmark: _Toc232953689][bookmark: _Toc516836559][bookmark: _Toc231566515][bookmark: _Toc231566641][bookmark: _Toc233624306]List of drawings
6.1. [bookmark: _Toc137798123][bookmark: _Toc229128326][bookmark: _Toc232953690][bookmark: _Toc516836560][bookmark: _Toc231566516][bookmark: _Toc231566642][bookmark: _Toc233624307]Drawings issued by the Employer
This is the list of drawings issued by the Employer at or before the Contract Date and which apply to this contract.
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The Lawns and Gardens areas are highlighted in Figure 1-5 and Table 1 below.
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